{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["ABX AIRCRAFT CONFIGURATION LIST","GENERAL NOTES & CATEGORY NOTES","REVISION HISTORY","NOTIFICATION LIST","REMOVED AIRCRAFT","FIN"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":3,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ABX AIRCRAFT CONFIGURATION LIST","index":0,"n_rows":42,"n_cols":90,"rows_kept":42,"cut":false,"hidden":false,"merged":[[0,3,0,4],[0,5,0,15],[0,81,0,89],[0,17,0,23],[0,24,0,27],[0,61,0,63],[0,46,0,53],[0,77,0,80],[0,29,0,36],[0,38,0,44],[0,55,0,60],[0,64,0,76]]}
["LAST MODIFIED DATE:",null,null,{"$f":"LASTSAVED()","v":"2025-04-17T09:24:19"},null,"AIRCRAFT DATA",null,null,null,null,null,null,null,null,null,null,null,"WEIGHT & BALANCE",null,null,null,null,null,null,"AIR CONDITIONING",null,null,null,"AUTOFLIGHT","COMMUNICATIONS",null,null,null,null,null,null,null,"ELECTRICAL","EQUIPMENT & FURNISHINGS",null,null,null,null,null,null,"FIRE PROTECTION","FUEL",null,null,null,null,null,null,null,"ICE & RAIN","INDICATING / RECORDING SYSTEM",null,null,null,null,null,"LANDING GEAR",null,null,"NAVIGATION",null,null,null,null,null,null,null,null,null,null,null,null,"WATER/WASTE",null,null,null,"CARGO & ACCESSORY COMPARTMENTS"]
["ABX “N” NUMBER","PREVIOUS\nNUMBER","SERIES","CARGO MOD","DATE\nMFG","SERIAL NUMBER","LINE","VARIABLE NUMBER","ENGINE","ORIGINAL\nOPERATOR","PAINT SCHEME","ETOPS\nCAPABLE","EURO\nOPS","FOQA","NEXTGEN\nFANS","APB\nWINGLET","FORECAST\nMODEL","OEW\nAOEW\nCG","WEIGHT\nGROUP","MTW","MTOW","MLW","MZFW","SABLE\nRESTRICTION","MAIN DECK\nNORMAL\nOR\nPERISHABLE","LOWER FWD\nAC SYSTEM\nOR\nNORMAL","LOWER AFT\nBULK CARGO","INSTRUMENT\nCOOLING\nMONITOR","AUTOPILOT COMPUTERS","SELCAL\nCODE","8.333\nCOMM","FM IMMUNITY","HF\nCOMM","SATCOM\nSYSTEM","SATCOM\nMSISDN","ACARS","PRINTER","HMG'S\nINSTALLED","SN\nSEATS","ACM\nSEATS","OVEN","SECURE\nCOCKPIT\nDOOR","ELT\nAUTO FIXED","ELT\nPORTABLE","AIRCRAFT\nULD","LWR CARGO\nDETECTOR\n BLOWER FANS","MAIN 1 or 2\nMAX VOLUME","MAIN 1 or 2\nMAX WEIGHT","CENTER\nMAX VOLUME","CENTER\nMAX WEIGHT","FQIS\nUNITS","CENTER\nOVERRIDE\nGFI","MAIN, AUX\nJETTISON\nGFI","FUEL\nJETTISON","ICE DETECT\nPRIMARY\nADVISORY\nNONE","CLASS E\nAURAL\nWARNING","WQAR\nuQAR","DFDAU","DFDR\nDATAFRAME","DFDR\nTYPE","IS&S\nFLAT PANEL","BRAKE TEMP\nMONITORING\nSYSTEM","WHEEL/BRAKE\nMFG\nBRAKE TYPE","NLG AXLE\nTHREAD\nCONFIG","STAND-BY\nINSTRUMENT\nSYSTEM","EGPWC\nPART NUMBER\n(See note 17 for Callout ID)","TAWS\nCLASS","MULTI-MODE\nRECEIVER\nGPS","FMC","FMC NAV\nDATABASE","EHS\nEXT SQT","MODE S","ADS-B\nOUT","XPONDERS","TCAS","IRU\nMag Tables","ALTERNATE\nVmo/Mmo\nSWITCH","LAVATORY\nMODULE","TOILET\nSYSTEM","LAV SVC PANEL(S)","WATER FOR HAND RINSING","CLS\nVENDOR","CLS\nCOMMERCIAL","CLS\nMILITARY","CLS\nENGINE","CLS\n16 FOOT","CARGO\nCOMPT\nCLASS","LOWER\nFORWARD","LOWER\nAFT","POWERED\nLWR CLS\nDEACTIVATED"]
["ATA-->","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",8,null,8,8,8,8,8,21,21,21,21,22,23,23,23,23,23,23,23,23,24,25,25,25,25,25,25,25,26,28,28,28,28,28,28,28,28,30,31,31,31,31,31,31,32,32,32,34,34,34,34,34,34,34,34,34,34,34,34,34,38,38,38,38,50,50,50,50,50,50,50,50,50]
["NOTES-->","-",1,2,null,null,null,null,null,null,3,null,22,null,"37, 40",56,null,6,54,7,7,7,7,13,49,35,null,27,45,null,20,20,15,null,49,39,16,26,10,11,null,32,4,5,64,31,null,8,null,8,null,25,52,null,30,12,18,44,null,41,14,29,42,50,66,17,43,null,62,null,19,null,63,36,21,"24, 51",33,57,58,"59, 60",61,34,"23, 65","9, 65","9, 47","9, 47",28,46,46,55]
["REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY ---------- REFERENCE ONLY"]
["219CY","G-VKN1","-383","BDSF","1989-05-04",24358,263,"VN153","PW4060","SAS","ABX-1B","YES/180","YES","YES","NO","NO","ABX-DHL 767-300","SEE\nNOTE","767-3A",413000,412000,320000,303000,"NONE","60-84 F (19-29 C)\n37-72 F (2-22 C)","43-77 F (6-25 C)\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","JQ-MP","YES","YES","YES\nCollins","AFIRS\nP/N 501-0001-1","See PMI ACU\nTech Desc","NO","NO",1,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.0 L","85200.0 LB\n38646.0 KG","Honeywell\nLB","SB\n767-28A0083","SB\n767-28A0085","NO","NONE","YES","WQAR with eADL","2233000-916","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Messier-Bugatti\nCarbon","External","ISU","965-0976-020-236-236","Class A","No","4052506-955 Pegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nACSS","Extended\n2015","NO","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","Ancra\n85000-10","A, C, D, E\n85000-10","Capable\nKit Not Purchased","Capable\nKit Not Purchased","Capable\nKit Not Purchased","Upper - E\nLower - C","K, P, Q, A, L, M","K, P, Q","YES"]
["220CY","EC-LKV","-383","BDSF","1991-03-01",24729,358,"VN157","PW4060","SAS","ABX-5","YES/180","YES","YES","NO","NO","ABX-DHL 767-300","SEE\nNOTE","767-3A",413000,412000,320000,303000,"NONE","60-84 F (19-29 C)\n37-72 F (2-22 C)","43-77 F (6-25 C)\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","HK-BP","YES","YES","YES\nCollins","AFIRS\nP/N 501-0001-1","See PMI ACU\nTech Desc","NO","NO",1,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.0 L","85200.0 LB\n38646.0 KG","Honeywell\nLB","SB\n767-28A0083","SB\n767-28A0085","YES","PRIMARY","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Messier-Bugatti\nCarbon","Internal","ESIS","965-0976-020-236-236","Class A","No","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nACSS","Extended\n2015","NO","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","Ancra\n85000-10","A, C, D, E\n85000-10","Capable\nKit Not Purchased","Capable\nKit Not Purchased","Capable\nKit Not Purchased","Upper - E\nLower - C","K, Q, A, L, M\nNo LD2","K, Q\nLD2 Aft 61R & 61L Only","YES"]
["226CY","EC-LKI","-383","BDSF","1992-01-15",26544,412,"VN168","PW4060","SAS","ABX-5","YES/180","YES","YES","NO","NO","ABX-DHL 767-300","SEE\nNOTE","767-3A",413000,412000,320000,303000,"NONE","60-84 F (19-29 C)\n37-72 F (2-22 C)","43-77 F (6-25 C)\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","KS-BD","YES","YES","YES\nCollins","NO","N/A","NO","NO",1,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.0 L","85200.0 LB\n38646.0 KG","Honeywell\nLB","SB\n767-28A0083","SB\n767-28A0085","YES","PRIMARY","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Messier-Bugatti\nCarbon","External","ISU","965-0976-020-236-236","Class A","No","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nACSS","Extended\n2015","NO","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","Ancra\n85000-10","A, C, D, E\n85000-10","Capable\nKit Not Purchased","Capable\nKit Not Purchased","Capable\nKit Not Purchased","Upper - E\nLower - C","K, P, Q, A, L, M","K, P, Q","YES"]
["290CM","JA619A",-381,"BDSF","2010-09-02",40564,993,"VS961","CF6-80C2B6F","ANA","DHL-1","YES/180","YES","YES","YES","YES","ABX-DHL 767-300","SEE\nNOTE","767-3I",413000,412000,326000,309000,null,"60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-703\n(P/N 822-1261-101)","AB-CM","YES","YES","YES","ICG ICS-220A\nP/N 710100-2","881652458547\n881652458688","Rockwell Collins\nCMU-900, 822-1239-151","YES",1,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES","5993.0 GAL\n22686 L","42,550.3 LB\n19,299 KG","11960.0 GAL\n45273.5 L","84916.0 LB\n38514.1 KG","Simmonds LB","Delivered from factory w/ intent of Boeing SB","Delivered from factory w/ intent of Boeing SB","YES","ADVISORY","YES","WQAR","2233000-816-1","767-6\n512 wps","Type 1A","5/11/5 DL","YES","Messier-Bugatti\nCarbon","External","Thales ISFD","965-0976-003-236-236  ","Class A","822-1821-001\nw/GPS","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","TPR-901\n822-1338-205","TCAS II 7.1\nCollins",2015,null,"IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","Ancra\n85000-30","A, C, D, E, G",null,"Installed\nConfig G",null,"Upper - E\nLower - C",null,null,"YES"]
["317CM","VH-OGC","-338","BDSF","1988-11-23",24317,246,"VN083","CF6-80C2B6","QAN","ABX-5","YES/180","YES","YES","NO","NO","ABX-ABX 767-300","SEE\nNOTE","767-3B",413000,412000,326000,309000,null,"60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","DG-AP","YES","YES","YES\nCollins","AFIRS\nP/N 501-0001-1","See PMI ACU\nTech Desc","NO","NO",3,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.0 L","85200.0 LB\n38646.0 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","NONE","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Messier-Bugatti\nCarbon","External","ESIS","965-0976-020-236-236  ","Class A","No","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","AAR\n59400-104","A, B, C, D, E, G, P\n(59400-110)","Installed (B)\n(Included with 59400-110)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, Q, A, L, M\nNo LD2","K, Q\nNo LD2","YES"]
["362CM","VH-OGB","-338","BDSF","1988-10-20",24316,242,"VN082","CF6-80C2B6","QAN","ABX-5","YES/180","YES","YES","NO","NO","ABX-DHL 767-300","SEE\nNOTE","767-3B",413000,412000,326000,309000,null,"60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","DK-JM","YES","YES","YES\nCollins","AFIRS\nP/N 501-0001-1","See PMI ACU\nTech Desc","NO","NO",3,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.0 L","85200.0 LB\n38646.0 KG","Honeywell\nLB","SB\n767-28A0083","SB\n767-28A0085","NO","NONE","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Messier-Bugatti\nCarbon","External","ESIS","965-0976-020-236-236     ","Class A","No","4052506-955 Pegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","AAR\n59400-104","A, C, D, E, G, P","Available - See Note\n(59170-101)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, Q, A, L, M\nNo LD2","K, Q\nNo LD2","YES"]
["363CM","VH-OGF","-338","BDSF","1989-09-05",24853,319,"VN086","CF6-80C2B6","QAN","White","YES/180","YES","YES","NO","NO","ABX-DHL 767-300","SEE\nNOTE","767-3B",413000,412000,326000,309000,null,"60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","EK-DG","YES","YES","YES\nCollins","AFIRS\nP/N 501-0001-1",null,"NO","NO",3,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.0 L","85200.0 LB\n38646.0 KG","Honeywell\nLB","SB\n767-28A0083","SB                   767-28A0085","YES","NONE","YES","WQAR with eADL","2233000-916","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Messier-Bugatti\nCarbon","Internal","ESIS","965-0976-020-236-236","Class A","822-1821-002\nw/GPS","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","AAR\n59400-104","A, C, D, E, G, P","Available - See Note\n(59170-101)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, Q, A, L, M\nNo LD2","K, Q\nNo LD2","YES"]
["364CM","VH-OGE","-338","BDSF","1989-09-05",24531,278,"VN085","CF6-80C2B6","QAN","ABX-5","YES/180","YES","YES","YES","NO","ABX-DHL 767-300","SEE\nNOTE","767-3B",413000,412000,326000,309000,null,"60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","EM-FG","YES","YES","YES\nCollins","ICG ICS-220A\nP/N 710100-2","881623455412\n881623455413","Rockwell Collins\nCMU-900, 822-1239-151","YES",3,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.0 L","85200.0 LB\n38646.0 KG","Honeywell\nLB","SB\n767-28A0083","SB                   767-28A0085","NO","NONE","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Messier-Bugatti\nCarbon","External","ESIS","965-0976-020-236-236","Class A","822-1821-002\nw/GPS","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","AAR\n59400-104","A, C, D, E, G, P","Available - See Note\n(59170-101)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, Q, A, L, M\nNo LD2","K, Q\nNo LD2","YES"]
["371CM","VH-OGO",-338,"BDSF","1994-08-26",25577,550,"VN095","CF6-80C2B6","QAN","DHL-1","YES/180","YES","YES","NO","NO","ABX-DHL 767-300","SEE\nNOTE","767-3D",381000,380000,320000,288000,"NONE","60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","QR-AG","YES","YES","YES\nCollins","NO","NO","NO","NO",3,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES","6010.0 GAL\n22750.3 L","42671.0 LB\n19355.2 KG","11900.0 GAL\n45046.4 L","84490.0 LB\n38321.0 KG","Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","NONE","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Messier-Bugatti\nCarbon","External","ESIS","965-0976-020-236-236","Class A","822-1152-002\nw/GPS","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","AAR\n59400-104","A, C, D, E, G, P","Available - See Note\n(59170-101)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, Q, A, L, M\nNo LD2","K, Q\nNo LD2","YES"]
["390CM","JA604A",-381,"BDSF","2002-06-27",32973,881,"VS722","CF6-80C2B6F","ANA","DHL-1","YES/180","YES","YES","YES","NO","ABX-DHL 767-300","SEE\nNOTE","767-3C",413000,412000,326000,309000,null,"60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","EP-BR","YES","YES","YES","ICG ICS-220A\nP/N 710100-2","881623441451\n881623455272","Rockwell Collins\nCMU-900, 822-1239-151","YES",1,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES","6010.0 GAL\n22750.3 L","42671.0 LB\n19353.6 KG","11960.0 GAL\n45273.5 L","84916.0 LB\n38514.1 KG","Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","ADVISORY","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","NO (EFIS)","YES","Messier-Bugatti\nCarbon","External","STANDARD","965-0976-003-236-236  ","Class A","822-1152-002\nw/GPS","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","Ancra\n85000-30","A, C, D, E, G",null,"Installed\nConfig G",null,"Upper - E\nLower - C",null,null,"YES"]
["391CM","JA606A",-381,"BDSF","2002-07-23",32975,883,"VS724","CF6-80C2B6F","ANA","DHL-1","YES/180","YES","YES","YES","NO","ABX-DHL 767-300","SEE\nNOTE","767-3C",413000,412000,326000,309000,null,"60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","ES-CL","YES","YES","YES","ICG ICS-220A\nP/N 710100-2","881623455895\n881623455978","Rockwell Collins\nCMU-900, 822-1239-151","YES",1,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES","6010.0 GAL\n22750.3 L","42671.0 LB\n19353.6 KG","11960.0 GAL\n45273.5 L","84916.0 LB\n38514.1 KG","Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","ADVISORY","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","NO (EFIS)","YES","Messier-Bugatti\nCarbon","External","STANDARD","965-0976-003-236-236","Class A","822-1152-002\nw/GPS","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","Ancra\n85000-30","A, C, D, E, G",null,"Installed\nConfig G",null,"Upper - E\nLower - C",null,null,"YES"]
["760CK","N760CK",-341,"BDSF","1990-02-01",24753,291,"VN232","CF6-80C2B6F","KAL","DHL-1","NOT YET","NO","YES",null,"NO","ABX-DHL 767-300","SEE\nNOTE","767-3B",413000,412000,326000,309000,null,"60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-703\n(P/N 822-1261-101)","FQ-EP","YES","YES","YES","Yes, but deactivated","N/A","YES","YES",1,0,4,"None","No Door","NO","Portable\nKannad, and in Life Rafts","YES","YES","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.9 L","85200.0 LB\n38646.0 KG","Honeywell LB","SB\n767-28A0083","SB\n767-28A0085","YES, but deactivated","NONE","YES","WQAR with eADL","2233000-816-1","767-3A\n256 wps","Type 1A","5/25/11","YES","Messier-Bugatti\nCarbon","Internal","ISU","965-0976-003-236-236  ","Class A","822-1152-004\nw/GPS","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","TPR-901\n822-1338-205","TCAS II 7.1\nCollins",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","AAR\n59400-104","A, C, D, E, G",null,"Installed\nConfig G",null,"Upper - E\nLower - C",null,null,"NO"]
["762CK","N762CK","-3P6","BDSF","1992-06-05",26236,436,"VN307","CF6-80C2B6","KAL","DHL-1","NOT YET","NO","YES",null,"NO","ABX-DHL 767-300","SEE\nNOTE","767-3B",413000,412000,326000,309000,null,"60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-703\n(P/N 822-1261-101)","JP-DG","YES","YES","YES","Yes, but deactivated","N/A","YES","YES",1,0,4,"None","No Door","NO","Portable\nKannad, and in Life Rafts","YES","YES","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.9 L","85200.0 LB\n38646.0 KG","Honeywell LB","SB\n767-28A0083","SB\n767-28A0085","YES","NONE","YES","WQAR with eADL","2233000-816-1","767-3A\n256 wps","Type 1A","5/25/11","YES","Messier-Bugatti\nCarbon","External","ISU","965-0648-008","Class A","822-1152-004\nw/GPS","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","TPR-901\n822-1338-205","ACSS\nT2CAS",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","AAR\n59400-104","A, C, D, E, G",null,"Installed\nConfig G",null,"Upper - E\nLower - C",null,null,"NO"]
["763CK","N763CK","-3P6","BDSF","1993-06-17",26233,501,"VN309","CF6-80C2B6","KAL","DHL-1","NOT YET","NO","YES",null,"NO","ABX-DHL 767-300","SEE\nNOTE","767-3C",413000,412000,326000,309000,null,"60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-703\n(P/N 822-1261-101)","CK-DG","YES","YES","YES","Yes, but deactivated","N/A","YES","YES",1,0,4,"None","No Door","NO","Portable\nKannad, and in Life Rafts","YES","YES","6010.0 GAL\n22750.3 L","42671.0 LB\n19355.2 KG","11900.0 GAL\n45046.4 L","84490.0 LB\n38324.0 KG","Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","NONE","YES","WQAR with eADL","2233000-816-1","767-3A\n256 wps","Type 1A","5/25/11","YES","Messier-Bugatti\nCarbon","External","ISU","965-0648-009","Class A","822-1152-004\nw/GPS","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","TPR-901\n822-1338-205","ACSS\nT2CAS",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","AAR\n59400-104","A, C, D, E, G",null,"Installed\nConfig G",null,"Upper - E\nLower - C",null,null,"YES"]
["764CK","N764CK","-3P6","BDSF","1994-05-25",26234,538,"VN313","CF6-80C2B6","KAL","DHL-1","NOT YET","NO","YES",null,"NO","ABX-DHL 767-300","SEE\nNOTE","767-3C",413000,412000,326000,309000,null,"60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-703\n(P/N 822-1261-101)","KL-DP","YES","YES","YES","Yes, but deactivated","N/A","YES","YES",1,0,4,"None","No Door","NO","Portable\nKannad, and in Life Rafts","YES","YES","6010.0 GAL\n22750.3 L","42671.0 LB\n19355.2 KG","11900.0 GAL\n45046.4 L","84490.0 LB\n38324.0 KG","Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","NONE","YES","WQAR with eADL","2233000-816-1","767-3A\n256 wps","Type 1A","5/25/11","YES","Messier-Bugatti\nCarbon","External","ISU","965-0648-008","Class A","822-1152-004\nw/GPS","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","TPR-901\n822-1338-205","ACSS\nT2CAS",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","AAR\n59400-104","A, C, D, E, G",null,"Installed\nConfig G",null,"Upper - E\nLower - C",null,null,"YES"]
["312AA","N/A",-223,"BDSF","1984-06-01",22315,94,"VA509","CF6-80A","AAL","ABX-5","YES/180","YES","YES","YES","NO","ABX-ABX 767-200","SEE\nNOTE","767-2A",352200,351000,283000,266000,"NONE","60-84 F (19-29 C)\n37-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","KM-AJ","YES","YES","YES\nCollins","ICG ICS-220A\nP/N 710100-2","881623441582\n881623441583","Rockwell Collins\nCMU-900, 822-1239-151","YES",1,3,2,"Microwave","Boeing","YES","Portable\nKannad","YES","NO","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Simmonds\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","NONE","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","NO","Honeywell\nSteel","Internal","ESIS","965-0976-003-236-236  ","Class A","822-1821-002\nw/GPS","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nAllied Signal\n(AAL)",2015,"YES","Boeing - Jamco\nL1","Boeing\nEnvirovac","Boeing AFT Active","Aircraft Press\nTank","AAR\n55973-123","A, C, D, E, G","Available - See Note\n(56414-102)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q","YES"]
["650GT","N702AX",-231,"P2S","1983-01-13",22566,29,"VA803","JT9D-7R4D","TWA","DHL-1","NO","NO","YES","NO","NO","ABX-DHL-767-200","SEE\nNOTE","767-2C",312000,310000,272000,253000,"Minor aft CG\nRestriction","66-77 F (19-25 C)\n36-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","BM-EK","NO","YES","NO","NO","NO","NO","NO",1,0,4,"None","Standard","YES","Portable\nKannad","NO","NO","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell LB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","NONE","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","Colllins Large Display System (LDS)","YES","Honeywell\nSteel","Internal","Thales ISFD","965-0976-003-239-239","Class A","No","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","Portable","None","None","AAR\n55973-103","A, C, D, E",null,null,null,"Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["651GT","N707AX",-231,"P2S","1983-07-16",22570,63,"VA807","JT9D-7R4D","TWA","DHL-1","NO","NO","YES","NO","NO","ABX-DHL-767-200","SEE\nNOTE","767-2C",312000,310000,272000,253000,"Minor aft CG\nRestriction","66-77 F (19-25 C)\n36-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","EK-HM","NO","YES","NO","NO","NO","NO","NO",1,0,4,"None","Standard","YES","Portable\nKannad","NO","NO","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell LB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","NONE","YES","WQAR","2233000-816-1","767-3A\n256 wps","Type 1A","NO (EFIS)","YES","Honeywell\nSteel","Internal","STANDARD","965-0976-003-236-236","Class A","No","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","Portable","None","None","AAR\n55973-103","A, C, D, E",null,null,null,"Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["744AX","N109DL","-232","BDSF","1983-05-10",22221,53,"VA309","CF6-80A2","DAL","ABX-2","NO","YES","YES","NO","NO","ABX-AMZ 767-200","SEE\nNOTE","767-2A",352200,351000,283000,266000,"NONE","66-77 F (19-25 C)\n36-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","LR-DM","YES","YES","YES\nHoneywell","NO","NO","NO","NO",0,3,2,"Microwave","Jamco","YES","Portable\nKannad","NO","NO","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG AEROSPACE","NO","ADVISORY","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Honeywell\nSteel","Internal","ESIS","965-0976-003-236-236","Class A","No","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","Boeing\nEnvirovac","Boeing AFT Active","Aircraft Press\nTank","AAR\n55973-103","A, C, D, E","Available - See Note\n56414-101","Available\n(57305-102)","Available\n(57305-102)","Upper - E\nLower - C","K, P, Q","K, P, Q","YES"]
["750AX","N115DA","-232","BDSF","1984-02-28",22227,83,"VA315","CF6-80A2","DAL","ABX-1A","NO","NO","YES","NO","NO","ABX-AMZ 767-200","SEE\nNOTE","767-2A",352200,351000,283000,266000,"NONE","66-77 F (19-25 C)\n36-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","LS-CG","YES","NO","YES\nHoneywell","NO","NO","NO","NO",0,3,2,"Microwave","Jamco","YES","Portable\nKannad","NO","NO","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","ADVISORY","YES","WQAR with eADL","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Honeywell\nSteel","Internal","ESIS","965-0976-003-236-236","Class A","No","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","Boeing\nEnvirovac","Boeing AFT Active","Aircraft Press\nTank","AAR\n55973-103","A, C, D, E","Available - See Note\n(56414-101)","Available\n(57305-102)","Available\n(57305-102)","Upper - E\nLower - C","K, P, Q","K, P, Q","YES"]
["767AX","JA8479","-281","P2S","1983-04-01",22785,51,"VB101","CF6-80A","ANA","ABX-1A","NO","YES","YES","NO","NO","ABX-ABX 767-200","SEE\nNOTE","767-2A",352200,351000,283000,266000,"NONE","66-77 F (19-25 C)\n36-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","AK-HR","YES","YES","YES\nHoneywell","AFIRS\nP/N 501-0001-1","See PMI ACU\nTech Desc","NO","NO",0,0,4,"Microwave","Standard","YES","Portable\nKannad","NO","NO","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG AEROSPACE","NO","ADVISORY","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","NO (EFIS)","YES","Honeywell\nSteel","Internal","STANDARD","965-0976-003-236-236","Class A","No","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","IAI\nMonogram","IAI FWD Left\nBoeing Aft Deact","Lav Faucet Tank","AAR\n55973-123","A, C, D, E, G","Available - See Note\n(56414-102)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["774AX","JA8483","-281","P2S","1983-09-01",22789,67,"VB105","CF6-80A","ANA","ABX-1B","NO","NO","NO","NO","NO","ABX-AMZ 767-200","SEE\nNOTE","767-2D",317000,315000,272000,253000,"Minor aft CG\nRestriction","66-77 F (19-25 C)\n36-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","EF-JM","NO","NO","NO","NO","N/A","NO","N/A",0,0,4,"None","Standard","YES","Portable\nKannad","NO","NO","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","ADVISORY","YES","WQAR with eADL","2233000-816","767-3A\n256 wps","Type 1A","NO (EFIS)","YES","Honeywell\nSteel","Internal","STANDARD","965-0976-003-236-236","Class A","No","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","IAI\nMonogram","IAI FWD Left\nBoeing Aft Deact","Lav Faucet Tank","AAR\n55973-123","A, C, D, E, G","Available - See Note\n(56414-102)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["783AX","JA8485","-281","P2S","1984-01-01",23016,80,"VB107","CF6-80A","ANA","DHL-1","NO","NO","NO","NO","NO","ABX-DHL 767-200","SEE\nNOTE","767-2D",317000,315000,272000,253000,"Minor aft CG\nRestriction","66-77 F (19-25 C)\n36-72 F (2-22 C)","No AC System\n40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","EK-DF","NO","NO","NO","NO","N/A","NO","N/A",0,0,4,"None","Standard","YES","Portable\nKannad","NO","NO","6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","ADVISORY","YES","WQAR","2233000-816","767-3A\n256 wps","Type 1A","NO (EFIS)","YES","Honeywell\nSteel","Internal","STANDARD","965-0976-003-236-236","Class A","No","4052506-955\nPegasus","GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","IAI\nMonogram","IAI FWD Left\nBoeing Aft Deact","Lav Faucet Tank","AAR\n55973-123","A, C, D, E, G","Available - See Note\n(56414-102)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["1013A","N1013A","-36N","BCF",null,30110,775,"VS323","CF6-80C2B6F","Atlas","Amazon","YES/180",null,"YES",null,"NO",null,null,null,413000,412000,326000,309000,null,null,null,null,"YES",null,"AD-LP",null,null,"YES","ICG ICS-220A\nP/N 710617-2",null,"YES (but no CPDLC)",null,1,0,4,null,"No Door","NO","Portable\nRescu 406S (2ea)",null,null,null,null,null,null,"Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","ADVISORY",null,"WQAR","2233000-816","767-3A\n256 wps",null,"Colllins Large Display System (LDS)",null,"Honeywell\nCarbon","Internal","Thales ISFD","965-0976-020-239-239",null,null,"4052506-955\nPegasus","GB7",null,"YES","YES",null,null,2015,null,null,null,null,null,"Ancra\n85250-20","A1, A2, M1, M2, E/R",null,"Installed\nConfig E/R",null,"Upper - E\nLower - E",null,null,"NO"]
["1093A","N1093A","-36N","BDSF",null,30111,776,"VS324","CF6-80C2B6F","Atlas","Amazon","YES/180",null,"YES",null,"NO",null,null,null,413000,412000,326000,309000,null,null,null,null,"YES",null,"AR-GJ",null,null,"YES","ICG ICS-220A\nP/N 710617-2",null,"Yes, but temporarily deactivated",null,1,0,4,null,"No Door","YES\n(ADT 406)","Portable\nRescu 406S (2ea)",null,null,null,null,null,null,"Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","ADVISORY",null,"WQAR","2233000-816","767-3A\n256 wps",null,"Colllins Large Display System (LDS)",null,"Honeywell\nCarbon","External","Thales ISFD","965-0976-020-239-239",null,null,"4052506-955\nPegasus","GB7",null,"YES","YES",null,"TCAS II 7.1 Honeywell",2015,null,null,null,null,null,"Ancra\n85000-10","A, C, D, E",null,null,null,"Upper - E\nLower - C",null,null,"NO"]
["1229A","N1229A","-306","BDSF",null,28884,738,"VS136","CF6-80C2B6F","Atlas","Amazon","YES/180",null,"YES",null,"NO",null,null,null,413000,412000,326000,309000,null,null,null,null,"YES",null,"BF-JP",null,null,"YES","ICG ICS-220A\nP/N 710617-2",null,"YES (but no CPDLC)",null,1,0,4,null,"No Door","YES","Portable\nRescu 406S (2ea)",null,null,null,null,null,null,"Simmonds LB","TDG\nAEROSPACE","TDG\nAEROSPACE","YES","PRIMARY",null,"WQAR","2233000-816-1","767-3A\n256 wps",null,"Colllins Large Display System (LDS)",null,"Honeywell\nCarbon","Internal","Thales ISFD","TBD",null,null,"4052506-955\nPegasus","GB7",null,"YES","YES",null,null,2015,null,null,null,null,null,"Ancra\n85000-10","A, C, D, E",null,null,null,"Upper - E\nLower - C",null,null,"NO"]
["1321A","N1321A","-306","BCF",null,27957,587,"VL891","CF6-80C2B6F","Atlas","Amazon","YES/180",null,"YES",null,"NO",null,null,null,413000,412000,326000,309000,null,null,null,null,"YES",null,"LM-JS",null,null,"YES","ICG ICS-220A\nP/N 710617-2",null,"YES (but no CPDLC)",null,1,0,4,null,"No Door","YES","Portable\nRescu 406S (2ea)",null,null,null,null,null,null,"Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","PRIMARY",null,"WQAR","2233000-816-1","767-3A\n256 wps",null,"Colllins Large Display System (LDS)",null,"Messier-Bugatti\nCarbon","External","Thales ISFD","965-0976-003-239-239",null,null,"4052506-955\nPegasus","GB7",null,"YES","YES",null,null,2015,null,null,null,null,null,"Ancra\n85250-20","A1, A2, M1, M2, E/R",null,"Installed\nConfig E/R",null,"Upper - E\nLower - E",null,null,"NO"]
["1327A","N1327A","-37D","BDSF",null,26328,637,"VL941","CF6-80C2B6F","Atlas","Amazon","YES/180",null,"YES",null,"NO",null,null,null,413000,412000,326000,309000,null,null,null,null,"YES",null,"BM-LQ",null,null,"YES","ICG ICS-220A\nP/N 710617-2",null,"YES (but no CPDLC)",null,1,0,4,null,"No Door","YES\n(B406)","Portable\nRescu 406S (2ea)",null,null,null,null,null,null,"Simmonds LB","TDG\nAEROSPACE","TDG\nAEROSPACE","YES","ADVISORY",null,"WQAR","2233000-816","767-3A\n256 wps",null,"Colllins Large Display System (LDS)",null,"Messier-Bugatti\nCarbon","External","Thales ISFD","965-0976-003-239-239",null,null,"4052506-955\nPegasus","GB7",null,"YES","YES",null,null,2015,null,null,null,null,null,"Ancra\n85000-10","A, C, D, E",null,null,null,"Upper - E\nLower - C",null,null,"NO"]
["1361A","N1361A","-31B","BCF",null,26265,570,"VL703","CF6-80C2B6F","Atlas","Amazon","YES/180",null,"YES",null,"YES",null,null,null,409000,408000,326000,309000,null,null,null,null,"YES",null,"JQ-FK",null,null,"YES","ICG ICS-220A\nP/N 710617-2",null,"YES (but no CPDLC)","YES",1,0,4,null,"No Door","YES\n(A06V2)","Portable\nRescu 406S (2ea)",null,null,null,null,null,null,"Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","NONE",null,"WQAR","2233000-816","767-3A\n256 wps",null,"Colllins Large Display System (LDS)",null,"Messier-Bugatti Carbon","External","Thales ISFD","965-0976-020-222-222",null,null,"4052506-955\nPegasus","GB7",null,"YES","YES",null,null,2015,null,null,null,null,null,"Ancra\n85250-20","A1, A2, M1, M2, E/R",null,"Installed\nConfig E/R",null,"Upper - E\nLower - E",null,null,"NO"]
["1427A","N1427A","-306","BCF",null,28098,607,"VL895","CF6-80C2B6F","Atlas","Amazon","YES/180",null,"YES",null,"NO",null,null,null,413000,412000,326000,309000,null,null,null,null,"YES",null,"CH-KM",null,null,"YES","ICG ICS-220A\nP/N 710617-2",null,"YES (but no CPDLC)",null,1,0,4,null,"No Door","NO","Portable\nRescu 406S (2ea)",null,null,null,null,null,null,"Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","PRIMARY",null,"WQAR","2233000-816","767-3A\n256 wps",null,"Colllins Large Display System (LDS)",null,"Messier-Bugatti Carbon","External","Thales ISFD","TBD",null,null,"4052506-955\nPegasus","GB7",null,"YES","YES",null,null,2015,null,null,null,null,null,"Ancra\n85250-20","A1, A2, M1, M2, E/R",null,"Installed\nConfig E/R",null,"Upper - E\nLower - E",null,null,"NO"]
["1489A","N1489A","-31K","BCF",null,27206,533,"VN952","CF6-80C2B6F","Atlas","Amazon","YES/180",null,"YES",null,"YES",null,null,null,409000,408000,326000,309000,null,null,null,null,"YES",null,"FP-ES",null,null,"YES","ICG ICS-220A\nP/N 710617-2",null,"YES (but no CPDLC)",null,1,0,4,null,"No Door","NO","Portable\nRescu 406S (2ea)",null,null,null,null,null,null,"Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","NONE",null,"WQAR","2233000-816-1","767-3A\n256 wps",null,"Colllins Large Display System (LDS)",null,"Messier-Bugatti Carbon","External","Thales ISFD","TBD",null,null,"4052506-955\nPegasus","GB7",null,"YES","YES",null,null,2015,null,null,null,null,null,"Ancra\n85250-20","A1, A2, M1, M2, E/R",null,"Installed\nConfig E/R",null,"Upper - E\nLower - E",null,null,"NO"]
["1499A","N1499A","-328","BCF",null,27428,586,"VN638","CF6-80C2B6F","Atlas","Amazon","YES/180",null,"YES",null,"NO",null,null,null,413000,412000,326000,309000,null,null,null,null,"YES",null,"BJ-FH",null,null,"YES","ICG ICS-220A\nP/N 710617-2\n(temporarily deact'd)",null,"Yes, but temporarily deactivated",null,1,0,4,null,"No Door","NO","Portable\nRescu 406S (2ea)",null,null,null,null,null,null,"Simmonds LB","SB\n767-28A0083","SB\n767-28A0085","YES","NONE",null,"WQAR","2233000-816","767-3A\n256 wps",null,"Colllins Large Display System (LDS)",null,"Honeywell\nCarbon","External","Thales ISFD","965-0976-003-239-239",null,null,"4052506-955\nPegasus","GB7",null,"YES","YES",null,null,2015,null,null,null,null,null,"Ancra\n85250-20","A1, A2, M1, M2, E/R",null,"Installed\nConfig E/R",null,"Upper - E\nLower - E",null,null,"NO"]
["1709A","N1709A","-375","BDSF",null,24086,248,"VN055","CF6-80C2B6F","Atlas","White","YES/180",null,"YES",null,"NO",null,null,null,413000,412000,326000,309000,null,null,null,null,"YES",null,"AJ-CH",null,null,"YES","ICG ICS-220A\nP/N 710617-2",null,"Yes, but temporarily deactivated",null,1,0,4,null,"No Door","YES\n(406AF)","Portable\nRescu 406S (2ea)",null,null,null,null,null,null,"Honeywell LB","SB\n767-28A0083","SB\n767-28A0085","NO","NONE",null,"WQAR","2233000-816","767-3A\n256 wps",null,"Colllins Large Display System (LDS)",null,"Honeywell\nCarbon","TBD","Thales ISFD","965-0976-020-239-239",null,null,"4052506-955\nPegasus","GB7",null,"YES","YES",null,null,2015,null,null,null,null,null,"AAR\n59400-104","A, C, D, E, G",null,null,null,"Upper - E\nLower - C",null,null,"NO"]
[]
["XXXXX","In Process of bieng Removed  from ABX Fleet"]
["XXXXX","In Process of being Added to ABX Fleet"]
[{"$f":"COUNTA(A6:A38)","v":33},"ABX Fleet Count"]

{"sheet":"GENERAL NOTES & CATEGORY NOTES","index":1,"n_rows":73,"n_cols":2,"rows_kept":73,"cut":false,"hidden":false,"merged":[]}
["GENERAL NOTES"]
["NOTE","DESCRIPTION"]
["A","Submit changes, corrections and revisions to abx.mtceng@abxair.com."]
["B","Click links within spreadsheet to open illustrations or additional documentation."]
[]
["CATEGORY NOTES"]
["NOTE","DESCRIPTION"]
[1,"Original series as delived to original operator."]
[2,"Passenger to Cargo aircraft modificaton vendor.\nBDSF - Bedek, Isreali Aircraft Industries (IAI), Supplemental Type Certificate\nBCSF - Boeing Converted Freighter, Type Certificate Admendment"]
[3,"Click link for example scheme.\nABX-1: White with stripes, gray belly, large logo, tail art.\nABX-1A: White with stripes, gray belly, large logo, no tail art, flag on tail.\nABX-1B: White with stripes, large logo, no tail art, flag on tail.\nABX-2: White with no stripes, gray belly, no logo, no tail art, flag on tail.\nABX-2A: White with no stripes, small logo on fuselage and tail, no tail art.\nABX-3: White with small logo on fuselage and tail, gray belly (315AA was the only aircraft painted like this)\nABX-4: Airborne Express Retro\nABX-5: 2021 Livery (White with stripes, red tail with art, large block logo)\nDHL-1: Yellow fuselage, red strips and logo.\nDHL-2: Half white (aft fuselage)/Half yellow (fwd fuselage) with red DHL logo."]
[4,"Fixed ELT,  EA 52548, STC ST02929AT"]
[5,"Life Rafts - Portable/Suvival ELT located in life rafts.\nPortable Kannad, Portable/Survival ELT. Kannad/Thales, PEA54091. Installed on forward side of smoke barrier.\nPortable Honeywell, Honeywell Rescu 406, Installed in cockpit."]
[6,"Copy link below and open in Internet Explorer or Windows Explorer. Enable Macros if prompted.\n    NOTE: Excel Macro Security must be set to Medium or Low. Open Excel-Tools-Macro-Security-Medium or Low.\n\\\\ILNSVR07\\iln04_data\\ACENG\\DATA\\WT_BAL\\QUERY.xls \nW&B QUERY File Data Columns\n   \"OEW\" and \"CG\" columns are current aircraft operating OEW weight and CG.\n   \"Current OEW\" and Current \"CG\" are Accumulated OEW and CG and not used for aircraft operations."]
[7,"Weight in Pounds"]
[8,"7.1 LB/GAL (0.8507 KG/L)"]
[9,"Capable - Aircraft can be configured to this configuration if CLS kit is purchased and installed. Also requires installation of placards and markings.\nAvailable - CLS Kits are available for installation in stock, but limited quantities.  Placards and markings must be verified.\n  59170-101 - B767-300 w/AAR CLS. ABX inventory 1 each.  ATI may have inventory if needed.\n  56414-101, -202 - B767-200 w/AAR.  Use -101 CLS Kit.  -101 & -012 CLS kits differ by CLS configuration placard. Components are the same.\nABX Rapid Change. B767-200SF Install/Remove\n  Rapid Change CLS system installed which can convert between Commercial and Military.\n     ABX-JEA-2550-0021 (formerly PMI Task JEA61782) INSTALL-RAPID CHANGE CLS MAIN DECK, 767-200SF\n     ABX-JEA-2550-0020 (formerly PMI Task JEA61781) REMOVE-RAPID CHANGE CLS MAIN DECK, 767-200SF\n  Convert Rapid Change Commercial to Military, Military to Commercial\n     ABX-JEA-2550-0017 (formerly PMI Task JEA57750) RELOCATE-CLS,COMMERCIAL RC2-MILITARY RC1,B767\n     ABX-JEA-2550-0016 (formerly PMI Task JEA57749) RELOCATE-CLS,MILITARY RC1-COMMERCIAL RC2,B767 \nB767-200SF Engine & 16 ft Pallet Kit Install/Remove\n  ABX-JEA-2550-0004 (formerly PMI Task JEA53140) INSTALL - ENGINE PALLET KIT, B767\n  ABX-JEA-2550-0005 (formerly PMI Task JEA53168) REMOVE - ENGINE PALLET KIT, B767\nB767-200SF Military CLS Kit Install/Remove\n  ABX-JEA-2550-0006 (formerly PMI Task JEA53500) INSTALL - MIL SYS KIT (CRAF CONFIG), B767\n  ABX-JEA-2550-0007 (formerly PMI Task JEA53558) REMOVE - MIL SYS KIT (CRAF CONFIG), B767\nB767-300BDSF Military CLS Kit Install/Remove\n  ABX-JEA-2550-0018 (formerly PMI Task JEA61338) RELOCATE-CLS,COMMERCIAL TO MILITARY,B767-300\n  ABX-JEA-2550-0019 (formerly PMI Task JEA61339) RELOCATE-CLS,MILITARY TO COMMERCIAL,B767-300"]
[10,"SN - Supernumerary Seats in Supernumerary Compartment"]
[11,"ACM - Additional Crew Member.  Additional seats in cockpit"]
[12,"Aural Warning - Class E Compartment (Maint Deck) aural warning for animal handlers."]
[13,"Minor Aft CG Restriction - Sable W&B system restricts aft CG limit slightly due to Cargo Lateral Imbalance (CLIM) calculation."]
[14,"XX/XX/XX - Refers to installed Flat Panel Configuration.  Integrated Flat Panel Display (IFPD) / Display control Panel (DCP)/ Data Concentrator Unit (DCU)\nDL - Data Loader Configuration\n5/19/11 - FPDS Config meets requirements of EASA STC 10036223"]
[15,"Collins - Originally equipped at delivery.\nHoneywell - Added by ABX. EA 23100015, EA 47797. Reactivation PEA23100022. Deactivation PEA23100021. AMES 39203ORD01.\nSTC ST01090SE & ST02130CH."]
[16,"Printer DI - Printer installed, but currently inoperative pending messaging software revision. "]
[17,"For Honeywell -236-236 EGPWS Computer:\nABX uses EGPWS Altitude Callout Menu 53 {Radio Altimeter (@2500), 1000, 100, 50 , 30, 20, 10}.\nCurrent software version (-236) installed by ABX-CEA-3444-0001 (formerly PMI CEA62023).  Issued to EGPWC by P/N & S/N.\n\nFor Honeywell -239-239 EGPWS Computer:\nABX uses EGPWS Altitude Callout Menu 53 {Radio Altimeter (@2500), 1000, 100, 50 , 30, 20, 10}.\nCurrent software version (-239) installed by and required for LDS STC.  No CEA yet created for installing this software.\n\nFor ACSS 965-0648-008/-009 T2CAS system EGPWS Mode 6 Altitude Callout:\nHas Callout ID (TBD)\nCurrent software version installed by ABX-EA-3446-0002."]
[18,"L3 Communications STC ST02776AT, EA 57858"]
[19,"EHS -Enhanced Surveillence\nEXT SQT - Extended Squitter\n\nRockwell Collins\nProvisional Wiring EA 34500008, EA 54318.  Install Activation EA 34500009, EA 54345\nSTCs ST01256WI-D, ST01901LA\nAvionics Group\nPEA34500004, PEA56200.  STC ST03559AT\nEnhanced Surveillence installed as part of ADS-B Out.  See Note 63"]
[20,"PEA34000056, PEA52641"]
[21,"All ABX Aircraft except 315AA, 219CY, 220CY, 226CY.\nRockwell Collins STC ST00393AT - TCAS II, STC ST00844WI-D - TCAS 7.0, STC ST00881WI-D - TCAS 7.1\nN315AA\nAAL Allied Signal STC SA3960SW-D - TCAS II 7.0, STC TCAS 7.1 Pending \n219CY, 220CY, 226CY\nHoneywell/ACSS STC SA5541NM -  TCAS II 7.0, ACSS STC ST02406LA - TCAS 7.1"]
[22,"Euro Ops requires ELS/EHS, 8.333 Comm, FM Immunity"]
[23,"Cargo Loading System installed on 793AX during PC2SF mod was removed from scrapped aircraft 799AX.  CLS is a different configuration from all other PC2SF aircraft."]
[24,"The Magnetic Variation Table Year listed indicates the IRU wire strapping configuration of the aircraft.\nExample - If aircraft is configured for a 1995 Magnetic Variation Table, the IRUs installed in the aircraft must support the same year."]
[25,"Automatic center tank override pump shutoff protection, GFI.\nUFI - Universal Fault Interrupter.  TDG Aerospace STC ST02284LA.  EA 57901, EA 28970001.\nSB 767-28A0083, Boeing modification."]
[26,"HMG - Hydraulic Motor Generator"]
[27,"Instrument cooling monitor panel installed on P6 panel."]
[28,"Cargo Compartment Class,  Class C - Extinguisher.  Class E - Depressurization."]
[29,"BTMS - Brake Tempature Monitor System."]
[30,"Aircraft listed as \"Primary\" require D06040-9 Yoke Checklist Placard.\nAircraft listed as \"Advisory\" or \"None\" require D06040-7 Yoke Checklist placard."]
[31,"Lower cargo compartment smoke detector system blower fans."]
[32,"Secure Cockpit Door.\nStandard - Original door installation, not secured.\nBoeing - Boeing SB 767-25-0327 secure cockpit door installation.\nJamco - Jamco STC ST01121SE secure cockpit door installation."]
[33,"Alternate Vmo/Mmo Switch Installation.  Vmo/Mmo - Maximum Operating Airspeed/Maximum Mach Airspeed"]
[34,"CLS P/N listed identifies the CLS that was purchased at time of cargo modification.  P/N may include a Military Kit that was not installed, but provided as a stocked kit."]
[35,"219CY & 220CY have supplemental air conditioning in lower forward compartment. "]
[36,"All transponder installations support Mode S and TCAS 7.1.  NXT-800 transponders support ADS-B Out."]
[37,"NEXTGEN - Next Generation Avionics or Next Generation Air Traffic Control, FANS - Future Air Navigation Systems.\nPENDING - Systems installed, but partially deactivated.  Waiting on Flight training and ARINC account for ATS services.  ACARS and printer deactivated. Prior OPC installed without ATS."]
[38,"ICG SatCom Installation - STC ST04139AT"]
[39,"ACARS Installation - STC ST04140AT"]
[40,"FMCS OPC PS40883821-906 Activates the following FANS Features:\n1. GLOBAL POSITIONING SYSTEM (GPS) ACTIVATION                \n2. REQUIRED NAVIGATION PERFORMANCE (RNP) ACTIVATION          \n3. RNP ENHANCEMENT PACKAGE                                   \n4. RNP APPROACH VALUE TO 0.3 NAUTICAL MILES (NM)             \n5. AIR TRAFFIC SERVICES DATA LINK (ATS DL)                   \n6. AIRLINE OPERATIONAL COMMUNICATIONS DATA LINK (AOC DL)     \n7. OFFSIDE ENGINE INDICATION AND CREW ALERTING SYSTEM (EICAS)\n8. OFFSIDE ELECTRONIC FLIGHT INSTRUMENT SYSTEM CONTROL PANEL \n9. FLIGHT MANAGEMENT COMPUTER (FMC) PRINTER INTERFACE        "]
[41,"FDR Type determined by IACO Annex 6"]
[42,"Wheel & Brake Combination Configuration and Brake Type.  Honeywell or Messier-Bugatti. Brakes - Steel or Carbon "]
[43,"TAWS - Terrain Awareness and Warning System.  Class A system required for Part 121 operators."]
[44,"DFDAU installed for expanded parameters.  DFDAU P/N 2233000-816 installed per STC ST01096CH.  DFDAU P/N 2233000-916 installed per STC ST09580SC to collect additonal data."]
[45,"Autopilot computer P/Ns include but not limited to P/Ns 622-4591-512, 622-8757-104, 822-1261-101, 622-8757-106, 622-8757-105"]
[46,"Lower cargo compartment ULD size codes.\n\n220CY\nRow 11 - LD3 \nRow 12 - LD3 \nRow 21 - LD2s or LD3\nRow 22 - LD2s \nRow 31 - LD3 \nRow 32 - LD3 \nRow 33 - LD3 \nRow 34 - LD3 \n\nRow 41 - LD3 \nRow 42 - LD3 \nRow 43 - LD3 \nRow 44 - LD3 \nRow 45 - LD3 \nRow 51 - LD2s or LD3 \nRow 61 - LD3 "]
[47,"793AX - Cargo Loading System installed was a removed and refurbished system from 799AX (SF) which did not include Engine or 16 Foot pallet provisoins."]
[48,"797AX Perishable Mod, Provisions Not Installed. Requires IAI SB 368-21-010. SB parts were provided to ABX after completion of cargo mod. "]
[49,"SatCom numbers for the ICG SatCom system will stay with the aircraft in a separate module.  Wingspeed and AFIRS numbers stay with the SatCom ACU."]
[50,"NLG Axle Thread Configuration - Internal or External.  Aircraft with External threads require installation of a Tang Axle Washer.  See ES02473. \n\nNLG Axle is part of NLG Inner Cylinder.  See below for which config each Inner Cylinder P/N is:\n\nINTERNAL threads:  162T1138-1, 162T1113-3\nEXTERNAL threads:  162T1138-3, -5"]
[51,"2015 MagVar installed by EA 60965, EA 34200001."]
[52,"Main, Aux & Jettison GFI.\nTDG Aerospace AMOC 75-3206-0001, STC ST02285LA. EA 61862, EA 28230005.\nSB 767-28A0085 Boeing Modification."]
[53,"Honeywell EGPWS Version. Installed by EGPWC P/N and S/N.  See JEA3444000X. New JEA issued with each database version."]
[54,"Aircraft Weight Groups are defined in the following W&B Reports:\n   46983WBR06 (for 767-200)\n   46983WBR02 (for 767-300)\nThese are weight groups for the W&B programs, and are not to be confused with the Configs, i.e., SF-A, SF-B, etc., that are given in the IAI Supp WBM."]
[55,"YES - Original Boeing Powered Lower Cargo Loading System Electrically Deactivated per ABX EO ABX-PEA-2550-0326 (DEACT-PWRD LOADING SYS,LWR CARGO COMP,B767). Aircraft Placarded.\nNO - Original Boeing Powered Lower Cargo Loading System Installed and Operational.    \nN/A - PC2SF Aircraft, Boeing Powered Cargo Loading System Not Installed. "]
[56,"Winglets installed per Aviation Partners Boeing (APB), STC ST01920SE"]
[57,"IAI-Dasell - lavatory module and toilet system installed by IAI cargo modification STC.\nBoeing Jamco - Original Boeing installed lav module."]
[58,"IAI Monogram - Toilet system installed by IAI cargo mod STC.\n     767-300BDSF installed in IAI Dasell cockpit lav module.\n     767-200P2S installed in original Boeing (Jamco) lav (L1) module.\nBoeing Rogerson - Original Boeing vacuum waste system installation."]
[59,"Boeing Aft Lav Service Panel - Under bulk cargo compartment is installed on all aircraft. Panel 163AL.\nBoeing AFT Deact - Lav Service Panel installed, but deactivated.  Deactivated on 767-300BDSF and 767-200P2S.\nBoeing AFT Active - Lav Service Panel installed and active.  Active on 767-200SF."]
[60,"IAI FWD Right - 767-300BDSF IAI Lav Service Panel installed on right side, forward of lower forward cargo door.\nIAI FWD Left - 767-200P2S IAI Lav Service Panel installed on the left side, above NLG doors. "]
[61,"Lav Faucet Tank - Water tank installed above sink in lav module. Installed by IAI cargo mod.  Not intended for drinking.\nAircraft Press Tank - Original Boeing installed water pressure tank and plumbing.  Not intended for drinking."]
[62,"750AX\nPegasus FMC P/Ns - 4052506-955\nRelated Software\nFMC OPS - 411-HNP-02C-10 (PS4083821-910)\nFMC OPC - 3415-BCG-005-W6 (240N2057-44)\nFMC FIDO - 3416-HNP-02E-11 (PS4084944-112)\nFMC AMI - 3416-HNP-02D-01 (242T102-6100)\nAircraft Modification Compiles with Boeing SB 767-34-0423 and 767-34-0566\nABX EO - EA 34600028, EA 65043"]
[63,"ADS-B Installation - STC ST04319CH, Mode S with Extended Squitter and Enhanced Surveillance\nProvision Only - Installs wiring for ADS-B system. Accomplished by EA 64240, EA 34530004.\n                           Equipment installation and activation per EA 64242, EA 34530005 required to complete system installation.\nADS-B System Installation - Installs complete system Accomplished by EA 64866, EA 34530006."]
[64,"ULD - Underwater Locator Device\nInstalled by ABX EO PEA23200002.  P/N 21435-00 (Novega)\nICAO Annex 6, Part I, Chapter 6.5.3.\n"]
[65,"The 59400-110 system will allow commercial and military to be carried without the need to configure or change locks."]
[66,"ESIS - Electronic Standby Instrument System (ESIS) is installed per STC ST02325CH with Flat Panel Display System (FPDS) per STC ST02165NY.\nISU - Integrated Standby Unit (ISU) per STC ST00399BO with Flat Panel Display System (FPDS) per STC ST02165NY.\nSTANDARD - Standard Boieng Standby Instrument Cluster."]

{"sheet":"REVISION HISTORY","index":2,"n_rows":158,"n_cols":2,"rows_kept":158,"cut":false,"hidden":false,"merged":[]}
["DATE","REVISION - CHANGE"]
["2012-11-05","Initial Release"]
["2012-11-14","Corrected ABX Rapid Change CLS. System was installed on 740AX after being removed from 742AX in May 2012."]
["2012-11-26","Changed Alternate Vmo/Mmo Switch from NO to Yes - 315AA, 740AX - 750AX."]
["2012-01-10","Messaging and Printer deactivated on 767AX, 219CY and 362CM"]
["2012-01-16","Added temperature ranges for main and loser decks in ATA 21."]
["2013-02-19","Added MODE S Column in ATA 34.\nAdded XPONDER Column in ATA 34\nAdded Note 36."]
["2013-07-10","798AX CLS converted from DHL Special (RC4) to Standard Commercial Configuration"]
["2013-07-15","797AX CLS converted from DHL Special (RC4) to Standard Commercial Configuration"]
["2013-07-29","TCAS 7.1 installed on 767AX\nUpdate Note 21 TCAS informatio to include new STCs."]
["2013-08-19","Added 364CM"]
["2013-10-07","TCAS 7.1 installed 745AX & 793AX."]
["2013-10-14","Corrected 750AX Configuration.  Was marked as Euro Ops.  Aircraft is not Euro Ops."]
["2013-11-04","Revised Ice Detect column to include \"Primary\", \"Advisory\" and \"None\"."]
["2014-01-08","Updated TCAS 7.1 Installatinos.\nRapid Change (RC1/RC2) removed from 750AX, installed on 767AX."]
["2014-02-07","Updated TCAS 7.1 Installatinos."]
["2014-03-07","Removed Rapid Change from 740AX installed on 745AX."]
["2014-03-11","Removed Rapid Change from 749AX installed on 744AX."]
["2014-05-16","Updated TCAS 7.1 Aircraft Installations\nUpdated ABX FOQA Aircraft"]
["2014-07-02","Added NextGen/FANS and ACARS columns.\nRevised 747AX configuration - NextGen/FANS modification. English to Metric. DFDAU & Dataframe.\nRevised 749AX Configuration - NextGen/FANS modification, DFDAU & Dataframe."]
["2014-07-18","Initiated entry for N226CY.\nAdded Wheel/Brake Config/Type, FDR Type and TAWS Class columns."]
["2014-08-01","Added column for Autoflight"]
["2014-08-06","TCAS 7.1 completed on 363CM"]
["2014-08-19","Corrected IS&S Flat Panel Display configuration numbers"]
["2014-09-09","Added lower cargo configurations.\nCorrected 797AX, Perishable System not installed.\nUpdated items for 226CY."]
["2014-09-19","Updated informaton for NextGen/FANS on 747AX, 749AX & 364CM.\nAdded SatCom numbers for ICG SatCom systems and note 49 to reference PMI for Wingspeed and AFIRS ACU for Satcom numbers.\nAdded additional information for 226CY."]
["2014-10-31","Corrected dataframe for 226CY.  364CM to ATI"]
["2014-11-24","Added IRU MagVar table year to 226CY"]
["2014-12-08","Updated EGPWS Altitude Callout from Menu Option 46 to 53\nAdded REMOVED AIRCRAFT Worksheet and transferred 364CM & 742AX."]
["2014-12-26","Added column for NLG Axle Thread Configuration."]
["2014-12-29","Updated aircraft with TCAS 7.1 upgrade. Removed 784AX & 786AX, xfer to Atlas.\n767AX added to FOQA Program."]
["2014-12-30","750AX added to FOQA Program."]
["2015-01-18","795AX added to FOQA Program."]
["2015-02-05","Removed 790AX and 747AX"]
["2015-02-24","Class E Aural Warning System installed on 752AX."]
["2015-03-09","LD3 Locks installed 226CY.\nTCAS 7.1 installed 219CY.\nRemoved 785AX."]
["2015-03-16","Updated EICAS OPS installations.  Version -08 installed."]
["2015-03-23","Verified extended Magnetitc Variation Tables installed on 219CY, 220CY, 226CY and noted in IRU Mag Table column.\nAdded General Note 51 for IRU Tables."]
["2015-04-17","Removed 749AX"]
["2015-05-26","362CM TCAS upgraded to 7.1"]
["2015-05-27","Added 371CM & 372CM "]
["2015-06-04","TCAS 7.1 installed on 745AX"]
["2015-06-22","Added column for Main, Aux, Jettison GFI configuration.\nAdded Note 52. Revised Note 51.\nUpdated items for 317CM and 372CM."]
["2015-07-09","Updated EGPWC column, added information to note 17."]
["2015-07-23","Added aircraft 312AA to list"]
["2015-08-03","Removed ABX Rapid Changed from 745AX, Installed on 767AX."]
["2015-08-24","Removed ABX Rapid Changed from 750AX, Installed on 740AX."]
["2015-08-31","Added column for EGPWS Database Version"]
["2015-10-05","Updated additional items for 312AA"]
["2015-10-12","Update information for 312AA.\nRemoved 745AX and 752AX.\nUpdate 315AA informaton due to FANS mod."]
["2015-10-20","Updated additional information for 371CM & 372CM"]
["2015-11-02","ABX Rapid Change CLS removed 740AX installed 312AA."]
["2015-12-26","2015 IRUs installed on 317CM"]
["2015-01-04","2015 IRUs installed on 750AX"]
["2016-01-21","Updated 372CM\nAdded Weight Group Column\nDeleted Owner and Operator columns\nCoded 315AA, aircraft scheduled to be leased\nAdded 749AX and updated, scheduled to be added to Ops Spec"]
["2016-03-22","Removed 315AA, Added 377CM"]
["2016-04-08","Added 384CM, 388CM, 389CM"]
["2016-05-16","Noted 749AX Deactivation of Satcom, ACARS and Printer"]
["2016-05-23","Added column for Muti-Mode Receiver GPS"]
["2016-06-02","Added IS&S Flat Panel Software Config for 312AA, 740AX, 744AX & 750AX."]
["2016-06-10","Added abx.gtscheduler@abxair.com to Notification List"]
["2016-07-06","Added 364CM to list. Being transfered form ATI to ABX."]
["2016-07-28","Added abxsafety@abxair.com to Notification List"]
["2016-08-23","Corrected aircraft S/N for 312AA"]
["2016-08-29","Changed registration numbers on pending 767-300 aircraft to reflect new Amazon numbers.\nAdded column CI to show which aircraft have the powered lower cargo loading system deactivated.\nConsolidated columns in Air Conditioning"]
["2016-08-30","220CY, LD2 locks installed in Aft positons 61R & 61L only."]
["2016-09-06","Removed Rapid Change CLS from 744AX, Installed on 750AX."]
["2016-09-09","219CY configured for Extended MagVar Tables."]
["2016-09-28","220CY configured for Extended MagVar Tables.\n364CM & 749AX ICG Satcoms Active, ACARS Deactivated pending ACARS subscription."]
["2016-10-03","226CY configured for Extended MagVar Tables."]
["2016-11-08","Updated 377CM (313AZ), Added 353AZ, Deleted 769AX.  Add Previous Number Column. Added APB Winglet Column"]
["2016-12-06","Removed aircraft 377CM (313AZ) will not be operated by ABX."]
["2016-12-07","Added ATA 38 Water/Waste section."]
["2016-12-08","Added ATA 47 Inert Gas System"]
["2016-12-20","Added 769AX (previously removed). Removed 337AZ, 353AZ & 359AZ."]
["2017-03-31","Removed 769AX from ABX fleet"]
["2017-04-13","Removed 793AX from ABX fleet"]
["2017-06-21","Corrected Cockpit door on 792AX from Standard to Boeing."]
["2017-07-20","Corrected fuel quantity system installed on 371CM from Honeywell to Simmons."]
["2017-10-06","EGPWS Database Version 487 added.  Installed by JEA64120."]
["2017-11-20","AFIRS Satcom and HF Installed on 794AX and Deactivated.\nInstalled for aircraft lease. "]
["2017-12-11","Added and tagged 752AX to list for transfer into ABX fleet.\nTagged 794AX for transfer out of ABX fleet.\nRemoved ATA 47 Inert Gas, no aircraft with system.\n"]
["2018-02-15","749AX - NextGen/FANS features enabled with ACARS activation, ACARS printer.\n794AX - Removed from ABX fleet. Leased to DHB."]
["2018-02-19","364CM - NextGen/FANS features enabled with ACARS activation, ACARS printer."]
["2018-02-26","752AX Added back to ABX fleet. Lease return from DHB."]
["2018-03-06","Removed 775AX from ABX fleet.\n750AX Remove Rapid Change CLS.\n740AX Install Rapid Change CLS"]
["2018-03-16","312AA NextGen/FANS equipment with ACARS, ICG SatCom, Pegasus FMC  installed and activated."]
["2018-03-19","Wingspeed SatCom system on 744AX permanetly deactivated.  Wingspeed system no longer supported or repairable."]
["2018-03-22","uQAR installed on aircraft 752AX and aircraft added to ABX FOQA program"]
["2018-04-09","Added SB and STC references in Note 32 for secure cockpit door installaitons."]
["2018-04-19","Added additional information to Note 9 to clarify CLS configurations."]
["2018-05-11","EGPWS Database Version 602 added.  Installed by JEA64579."]
["2018-05-30","Aircraft N797AX painted in current ABX Air paint scheme."]
["2018-06-15","EGPWS Database Version 602 added.  Installed by JEA64699."]
["2018-06-19","Wingspeed SatCom system on 750AX permanetly deactivated.  Wingspeed system no longer supported or repairable."]
["2018-08-08","EGPWS Database Version 604 added.  Installed by JEA64855."]
["2018-09-14","Removed 787AX, 788AX, 792AX."]
["2018-10-26","Removed 773AX"]
["2018-11-13","Pegasus FMC installed on 750AX per EO EA EA 65043."]
["2018-11-15","Removed the follwoing columns:\nEICAS OPS/OPC\nFMC OPS/OPC\nFlat Panel Software\nRefer to ABX Aircraft Software Configuraiont Lists"]
["2018-11-17","Pegasus FMC installed on 740AX per EO EA EA 65043."]
["2018-12-05","Pegasus FMC installed on 744AX per EO EA EA 65043.\nFPDS upgraded on 744AX to 5/11/5 DL per EA 60979."]
["2018-12-05","EGPWS Database current version 606. JEA65146."]
["2018-12-14","Added ADS-B column, ATA 34."]
["02/04.2019","ADS-B activated on 797AX.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-02-04","ADS-B activated on 219CY.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-02-05","ADS-B activated on 744AX.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-02-07","Rapid Change CLS installed on 797AX."]
["2019-02-07","N219CY DFDAU changed to P/N 2233000-816 with 767-3A Dataframe"]
["2019-02-17","ADS-B activated on 362CM.  ADS-B Out, Extended Squitter, Enhanced Surveillence"]
["2019-02-19","Flat Panel Display System installed on 220CY 5/11/5 DL"]
["2019-02-25","ADS-B activated on 749AX.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-02-28","ADS-B activated on 364CM.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-03-05","ADS-B activated on 774AX.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-03-14","ADS-B activated on 220CY.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-03-19","ADS-B activated on 752AX.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-03-26","ADS-B activated on 768AX.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-04-15","Added column ATA 25 for aircraft Underwater Locator Device (ULD).\nULD installed on aircraft 312AA."]
["2019-04-16","ADS-B activated on 363CM.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-04-19","ADS-B activated on 795AX.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-04-19","Aircraft Underwater Locator Device (ULD) Installed on aircraft 364CM."]
["2019-04-16","ADS-B installed and activated on 740AX.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-05-15","Removed GFSFC group email, added ABXFC group email to Notification List."]
["2019-05-30","Rapid Change CLS removed from 797AX."]
["2019-05-31","ADS-B installed and activated on 767AX.  ADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-07-01","ADS-B installed and activated on 226CY and 750AX.\nADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-07-15","Corrected water/watse system for several 767-200 aircraft."]
["2019-09-16","ADS-B installed and activated on 317CM, 312AA and 783AX.\nADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2019-09-16","ULD installed on 317CM"]
["2019-09-19","317CM, installed Commercial & Military Combo CLS 59400-110."]
["2019-11-01","HF system removed from 798AX per management request."]
["2019-11-01","ADS-B installed and activated on 371CM.\nADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2020-01-21","Deleted EGPWS Terrian Database Column"]
["2020-01-31","ADS-B installed and activated on 372CM.\nADS-B Out, Extended Squitter, Enhanced Surveillance"]
["2020-03-06","Added \"STAND-BY INSTRUMENT SYSTEM\" column in ATA 34 to indicate install of \"ESIS\", \"ISU\", or \"STANDARD\"\nUpdated N219CY to Flat Panel Display System installed per STC ST02165NY.\nUpdated N219CY to ISU installed per STC STC ST00399BO."]
["2020-03-27","Updated N226CY to Flat Panel Display System installed per STC ST02165NY.\nUpdated N226CY to ISU installed per STC STC ST00399BO."]
["2020-05-21","768AX DFDAU Dataframe updated to 767-3A."]
["2020-05-22","774AX Pegasus FMC Installed."]
["2020-05-29","768AX Pegasus FMC installed.\nRemoved 798AX.\nMarked 363CM for removal from ABX fleet.  Aircraft to be leased to another operator."]
["2020-06-08","783AX Pegasus FMC installed."]
["2020-06-30","Removed 363CM from list"]
["2020-07-13","Aircraft ULD installed 372CM"]
["2020-07-21","Aircraft ULD installed 371CM"]
["2020-08-03","Aircraft ULD installed 219CY"]
["2020-08-10","Added WQAR (Wireless Quick Access Recorder installation information to ATA 31."]
["2020-08-10","Aircraft ULD installed 226CY"]
["2020-08-20","795AX Pegasus FMC installed.\n795AX WQAR installed.\n744AX WQAR installed and Dataframe to 767-3A.\n220CY Aircraft ULD installed.\n362CM Aircraft ULD installed"]
["2020-10-09","752AX removed from ABX Ops."]
["2020-11-16","Added N742AX to Configuration List"]
["2021-01-07","Corrected POWERED LWR CLS DEACTIVATED to NO for 364CM, 371CM, 372CM until REQ ABX-PEA-2550-0326 (DEACT-PWRD LOADING SYS,LWR CARGO COMP,B767) is accomplished."]
["2020-01-07","Removed N742AX"]
["2021-03-01","WQAR installed N219CY"]
["2021-03-25","220CY - Pegasus FMC installed, FQIS change to English units. WQAR installed.\n767AX - Pegasus FMC installed.WQAR installed."]
["2012-04-12","797AX Pegasus FMC installed."]
["2021-05-03","Added 767-200 N650GT and N651GT"]
["2021-05-21","317CM Pegasus FMC installed.  FQIS change to English units. WQAR installed."]
["2021-08-31","Added SELCAL code to N651GT (-engwc)"]
["2022-04-03","Several updates based upon recent mods, i.e., kg-to-lbs, wQAR, Pegasus, DFDR dataframe, M-B carbon brakes.  Added more information for 650GT & 651GT.  Added 390CM & 391CM and filled in as much info as we know. (-engwc)"]

{"sheet":"NOTIFICATION LIST","index":3,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["CONFIGURATION LIST REVISION/CHANGE NOTIFICATION"]
["GROUP/DEPARTMENT EMAIL","GROUP/DEPARTMENT"]
["ABX.MTCENG@ABXAIR.COM","ABX Engineering"]
["ABXMC@ABXAIR.COM","ABX Maintenance Control"]
["ABXFC@ABXAIR.COM","ABX Flight Control"]
["ABXSC@ABXAIR.COM","ABX System Control"]
["FlightManagement@abxair.com","ABX Flight Management"]
["abx.gtscheduler@abxair.com","ABX Ground Department"]
["abxsafety@abxair.com","ABX Safety Department"]
["Brian.L.Byers@faa.gov","FAA Principal Avionics Inspector (PAI)"]
["Charles.G.Dault@faa.gov","FAA Principal Maintenance Inspector (PMI)"]
["weight@airbornemx.com","AMES W&B group"]
[]
["ABX.MTCENG <ABX.MTCENG@abxair.com>; ABXMC <ABXMC@abxair.com>; abxfc <abxfc@abxair.com>; ABXSC <ABXSC@abxair.com>; FlightManagement <FlightManagement@abxair.com>; ABX GTScheduler <ABX.GTScheduler@abxair.com>; abxsafety <abxsafety@abxair.com>; david.utchel@faa.gov; Catherine.Rettich@abxair.com"]

{"sheet":"REMOVED AIRCRAFT","index":4,"n_rows":41,"n_cols":104,"rows_kept":41,"cut":false,"hidden":false,"merged":[[0,90,0,93],[0,95,0,103],[0,51,0,59],[0,72,0,89],[0,4,0,5],[0,6,0,16],[0,19,0,25],[0,26,0,32],[0,34,0,41],[0,69,0,71],[0,61,0,68],[0,43,0,49]]}
["LAST MODIFIED DATE:",null,null,null,{"$f":"LASTSAVED()","v":"2025-04-17T09:24:19"},null,"AIRCRAFT DATA",null,null,null,null,null,null,null,null,null,null,null,null,"WEIGHT & BALANCE",null,null,null,null,null,null,"AIR CONDITIONING",null,null,null,null,null,null,"AUTOFLIGHT","COMMUNICATIONS",null,null,null,null,null,null,null,"ELECTRICAL","EQUIPMENT & FURNISHINGS",null,null,null,null,null,null,"FIRE PROTECTION","FUEL SYSTEM",null,null,null,null,null,null,null,null,"ICE & RAIN","INDICATING / RECORDING SYSTEM",null,null,null,null,null,null,null,"LANDING GEAR",null,null,"NAVIGATION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WATER/WASTE",null,null,null,"NGS","CARGO & ACCESSORY COMPARTMENTS"]
["ABX “N” NUMBER","PREVIOUS\nNUMBER","SERIES","CARGO MOD","DATE MFG","SERIAL NUMBER","LINE","VARIABLE NUMBER","ENGINE","OWNER","OPERATOR","ORIGINAL\nOPERATOR","PAINT SCHEME","ETOPS","EURO\nOPS","FOQA","NEXTGEN\nFANS","APB\nWINGLET","FORECAST\nMODEL","OEW\nAOEW\nCG","WEIGHT GROUP","MTW","MTOW","MLW","MZFW","SABLE\nRESTRICTION","PERISHABLE\nMODE ECS","MAIN DECK\nNORMAL","MAIN DECK\nPERISHABLE","FORWARD LOWER\nNORM OR PERISHABLE","AFT/BULK LOWER\nNORM OR PERISHABLE","LOWER FWD AC SYSTEM or NORMAL","INSTRUMENT\nCOOLING\nMONITOR","AUTOPILOT COMPUTERS","SELCAL\nCODE","8.333\nCOMM","FM IMMUNITY","HF\nCOMM","SATCOM\nSYSTEM","SATCOM\nMSISDN","ACARS","PRINTER","HMG'S\nINSTALLED","SN\nSEATS","ACM\nSEATS","OVEN","SECURE\nCOCPIT\nDOOR","ELT\nAUTO FIXED","ELT\nPORTABLE","AIRCRAFT ULD","LWR CARGO\nDETECTOR\n BLOWER FANS","FUEL TANKS","USABLE\nFUEL TANK QUANTITY","USABLE\nFUEL TANK\nWEIGHT","CENTER\nMAX VOLUME","CENTER\nMAX WEIGHT","FQIS\nUNITS","CENTER\nOVERRIDE\nUFI","MAIN, AUX JETTISON GFI","FUEL\nJETTISON","ICE DETECT\nPRIMARY\nADVISORY\nNONE","CLASS E\nAURAL\nWARNING","EICAS\nOPS","EICAS\nOPC","WQAR\nuQAR","DFDAU","DFDR\nDATAFRAME","DFDR\nTYPE","IS&S\nFLAT\nPANEL","BRAKE TEMP\nMONITORING\nSYSTEM","WHEEL/BRAKE\nMFG\nBRAKE TYPE","NLG AXLE\nTHREAD\nCONFIG","STAND-BY\nINSTRUMENT\nSYSTEM","IS&S\nFLAT PANEL","FLAT\nPANEL\nSOFTWARE","EGPWS\nPART NUMBER\nTYPE/ALTITUDE","?","TAWS\nCLASS","?","MULTI-MODE RECEIVER GPS","FMC","FMCS\nOPS","FMC NAV\nDATABASE","ELE/EHS","MODE S","ADS-B\nOUT","XPONDERS","TCAS","IRU\nMag Tables","ALTERNATE\nVmo/Mmo\nSWITCH","LAVATORY\nMODULE","TOILET\nSYSTEM","LAV SVC PANEL(S)","WATER FOR HAND RINSING","NITROGEN\nGENERATING\nSYSTEM","CLS\nVENDOR","CLS\nCOMMERCIAL","CLS\nMILITARY","CLS\nENGINE","CLS\n16 FOOT","CARGO\nCOMPT\nCLASS","LOWER\nFORWARD","LOWER\nAFT","POWERED\nLWR CLS\nDEACTIVATED"]
["ATA-->",null,"-","-","-","-","-","-","-","-",null,"-","-","-","-","-","-","-","-",8,8,8,8,8,8,8,21,21,21,21,21,null,21,22,23,23,23,23,23,23,23,23,24,25,25,25,25,25,25,null,26,28,28,28,28,28,28,28,28,28,30,31,31,31,31,31,31,31,31,32,32,32,34,34,34,34,null,34,null,34,34,34,34,34,34,34,34,34,34,34,38,38,38,38,47,50,50,50,50,50,50,50,50,50]
["NOTES-->",null,1,2,null,null,null,null,null,null,null,null,3,null,22,null,"37, 40",56,null,6,54,7,7,7,7,13,48,null,null,35,null,null,27,45,null,20,20,15,null,49,39,16,26,10,11,null,32,4,5,null,31,8,null,null,null,8,null,25,52,null,30,12,null,null,18,44,null,41,14,29,42,null,14,null,null,17,null,43,null,null,null,40,null,19,null,63,36,21,24,32,57,58,"59, 60",61,null,34,23,9,"9, 47","9, 47",28,46,46,55]
[]
["742AX",null,"-232","BDSF","1983-01-19",22217,27,"VA305","CF6-80A2","CAM","CargoJet","DAL","ABX-1","NO","YES","NO","NO",null,null,"SEE\nNOTE",null,352200,351000,283000,266000,"NONE","YES","66-77 F (19-25 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)","40-50 F (4.5-10 C)",null,"NO","Rockwell Collins\nModels FCC-701, -702, -703","LR-CM","YES","YES","YES\nHoneywell","Wingspeed\n1000608-ACU-A","See PMI ACU\nTech Desc","NO","YES",0,3,2,"Microwave","Jamco","YES","Portable\nKannad",null,"NO","Main 1 & 2\nCenter-LR","16700 GAL","118570 LB",null,null,"Honeywell\nLB","TDG\nAEROSPACE",null,"NO","ADVISORY","YES","3176-COL-DE0-05\nPost SB 31-180","310C-BCG-006-M3\nPost SB 31-0098","QAR201-02-00","2233000-816","767-4\n64 wps","Type !A",null,"YES","Honeywell\nSteel",null,null,"1/1/1","PENDING","965-0976-003-216- 216\n221/53",null,"Class A",null,null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","YES\nCollins","YES",null,"LH & RH\n822-1338-003","TCAS II 7.1\nCollins",1980,"YES",null,null,null,null,null,"AAR\n55973-103","A, C, D, E\n55973-103","Available\n56414-101","Available\n57305-102","Available\n57305-102","Upper - E\nLower - C","K, P, Q","K, P, Q"]
["784AX",null,"-281","P2SD","1984-03-01",23017,82,"VB108","CF6-80A","DHL","Atlas","ANA","DHL-1","NO","NO","NO","NO",null,null,"SEE\nNOTE",null,317000,315000,272000,253000,"Minor aft CG\nRestriction","YES","66-77 F (19-25 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)","40-50 F (4.5-10 C)",null,"NO","Rockwell Collins\nModels FCC-701, -702, -703","EL-DM","NO","NO","NO","NO","N/A","NO","N/A",0,0,4,"None","Standard","NO","Portable\nKannad",null,"NO","Main 1 & 2\nCenter-LR","16700 GAL","118570 LB",null,null,"Honeywell\nLB","TDG\nAEROSPACE",null,"NO","ADVISORY","YES","3176-COL-DE0-05\nPost SB 31-180","310B-BCG-00M-20\nPost SB 31-0098","N/A","2233000-816","767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"NO","N/A","965-0976-003-216- 216\n221/53",null,"Class A",null,null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","NO","YES",null,"LH 822-1338-002\nRH 066-01127-1301",null,1980,"YES",null,null,null,null,null,"AAR\n55973-123","A, C, D, E, G","Available\n56414-101","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q"]
["786AX",null,"-281","P2SC","1984-05-01",23019,85,"VB110","CF6-80A","DHL","Atlas","ANA","DHL-1","NO","NO","NO","NO",null,null,"SEE\nNOTE",null,312000,310000,272000,253000,"Minor aft CG\nRestriction","YES","66-77 F (19-25 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)","40-50 F (4.5-10 C)",null,"NO","Rockwell Collins\nModels FCC-701, -702, -703","EL-GM","NO","NO","NO","NO","N/A","NO","N/A",0,0,4,"None","Standard","NO","Portable\nKannad",null,"NO","Main 1 & 2\nCenter-LR","16700 GAL","118570 LB",null,null,"Honeywell\nLB","TDG\nAEROSPACE",null,"NO","ADVISORY","YES","3176-COL-DE0-05\nPost SB 31-180","310B-BCG-00M-20\nPost SB 31-0098","N/A","2233000-816","767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"NO","N/A","965-0976-003-216- 216\n221/53",null,"Class A",null,null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","NO","YES",null,"LH 822-1338-002\nRH 066-01127-1301",null,1980,"YES",null,null,null,null,null,"AAR\n55973-123","A, C, D, E, G","Available\n56414-101","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q"]
["790AX",null,"-281","P2SC","1984-11-27",23140,106,"VB114","CF6-80A","DHL","Atlas","ANA","DHL-1","NO","NO","NO","NO",null,null,"SEE\nNOTE",null,312000,310000,272000,253000,"Minor aft CG\nRestriction","YES","66-77 F (19-25 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)","40-50 F (4.5-10 C)",null,"NO","Rockwell Collins\nModels FCC-701, -702, -703","AH-CG","NO","NO","NO","AFIRS\nP/N 501-0001-1","See PMI ACU\nTech Desc","NO","NO",0,0,4,"None","Boeing","YES","Portable\nKannad",null,"NO","Main 1 & 2\nCenter-LR","16700 GAL","118570 LB",null,null,"Honeywell\nLB","TDG\nAEROSPACE",null,"NO","ADVISORY","YES","3176-COL-DE0-05\nPost SB 31-180","310B-BCG-00M-20\nPost SB 31-0098","N/A","2233000-816","767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"NO","N/A","965-0976-003-216- 216\n221/53",null,"Class A",null,null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","NO","YES",null,"LH 822-1338-002\nRH 066-01127-1301",null,1980,"YES",null,null,null,null,null,"AAR\n55973-123","A, C, D, E, G","Available\n56414-101","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q"]
["747AX",null,"-232","BDSF","1983-12-08",22224,76,"VA312","CF6-80A2","CAM","West Atlantic","DAL","White","NO","YES","YES","YES\nFANS DEACT",null,null,"SEE\nNOTE",null,352200,351000,283000,266000,"NONE","YES","66-77 F (19-25 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)","40-50 F (4.5-10 C)",null,"NO","Rockwell Collins\nModels FCC-701, -702, -703","LR-FG","YES","YES","YES\nHoneywell","ICG\nModel  ICS-220A\nP/N 710100-2","881623455435\n881623455436","Rockwell Collins\nCMU-900\n822-1239-151","YES",0,3,2,"Microwave","Jamco","YES","Portable\nKannad",null,"NO","Main 1 & 2\nCenter-LR","16700 GAL","118570 LB",null,null,"Honeywell\nLB","TDG\nAEROSPACE",null,"NO","ADVISORY","YES","3176-COL-DE0-05\nPost SB 31-180","TBD\nPost SB 31-0098","QAR200-02-00","2233000-816","B767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"5/19/11 DL","PENDING","965-0976-003-216- 216\n221/53",null,"Class A",null,null,"4052506-955\nS242T102-455\nPegasus","PS40883821-906\nFANS","A, B, C, D, E, G, P\n(59400-110)","YES\nCollins","YES",null,"LH & RH\n822-1338-003",null,2015,"YES",null,null,null,null,null,"AAR\n55973-103","A, C, D, E\n55973-103","Available\n56414-101","Available\n57305-102","Available\n57305-102","Upper - E\nLower - C","K, P, Q","K, P, Q"]
["749AX",null,"-232","BDSF","1984-01-25",22226,78,"VA314","CF6-80A2","CAM","ABX","DAL","ABX-1","NO","YES","YES","YES\nFANS DEACT",null,null,"SEE\nNOTE",null,352200,351000,283000,266000,"NONE","YES","66-77 F (19-25 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)","40-50 F (4.5-10 C)",null,"NO","Rockwell Collins\nModels FCC-701, -702, -703","LS-AF","YES","YES","YES\nHoneywell","ICG\nModel  ICS-220A\nP/N 710100-2","881623455410\n881623455411","Rockwell Collins\nCMU-900\n822-1239-151","YES",0,3,2,"Microwave","Jamco","YES","Portable\nKannad",null,"NO","Main 1 & 2\nCenter-LR","16700 GAL","118570 LB",null,null,"Honeywell\nLB","TDG\nAEROSPACE",null,"NO","ADVISORY","YES","317B-COL-DE0-08 POST SB 31-0295","TBD\nPost SB 31-0098","QAR201-02-00","2233000-816","767-4\n64 wps","Type !A",null,"YES","Honeywell\nSteel","Internal",null,"5/11/5 DL","PENDING","965-0976-003-216- 216\n221/53",null,"Class A",null,null,"4052506-955\nS242T102-455\nPegasus","PS40883821-906\nFANS","GB7","YES\nCollins","YES",null,"LH & RH\n822-1338-003",null,2015,"YES",null,null,null,null,null,"AAR\n55973-103","A, C, D, E\n55973-103","Available\n56414-101","Available\n57305-102","Available\n57305-102","Upper - E\nLower - C","K, P, Q","K, P, Q"]
["785AX",null,"-281","P2SC","1984-04-01",23018,84,"VB109","CF6-80A","DHL","White","ANA","DHL-1","NO","NO","NO","NO",null,null,"SEE\nNOTE",null,312000,310000,272000,253000,"Minor aft CG\nRestriction","YES","66-77 F (19-25 C)","36-72 F (2-22 C)","EK-DG","40-50 F (4.5-10 C)",null,"NO","Rockwell Collins\nModels FCC-701, -702, -703",null,"NO","NO","NO","AFIRS\nP/N 501-0001-1","See PMI ACU\nTech Desc","NO","NO",0,0,4,"None","Standard","PENDING","Portable\nKannad",null,"NO","Main 1 & 2\nCenter-LR","16700 GAL","YES",null,null,"Honeywell\nLB","TDG\nAEROSPACE",null,"NO","ADVISORY","YES","3176-COL-DE0-05\nPost SB 31-180","310F-BCG-013-K2\nPost SB 767-34-0703","N/A","2233000-816","767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"NO","N/A","965-0976-003-216- 216\n221/53",null,"Class A",null,null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","NO","YES",null,"LH 822-1338-002\nRH 066-01127-1301",null,1980,"YES",null,null,null,null,null,"AAR\n55973-123","A, C, D, E, G","Available\n56414-101","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q"]
["745AX",null,"-232","BDSF","1983-06-04",22222,56,"VA310","CF6-80A2","CAM","ABX","DAL","ABX-1","NO","YES","YES","NO",null,null,"SEE\nNOTE",null,352200,351000,283000,266000,"NONE","YES","66-77 F (19-25 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)","40-50 F (4.5-10 C)",null,"NO","Rockwell Collins\nModels FCC-701, -702, -703","LR-EJ","YES","YES","YES\nHoneywell","NO","NO","NO","YES",0,3,2,"Microwave","Jamco","YES","Portable\nKannad",null,"NO","Main 1 & 2\nCenter-LR","16700 GAL","118570 LB",null,null,"Honeywell\nLB","TDG\nAEROSPACE",null,"NO","ADVISORY","YES","317B-COL-DE0-08 POST SB 31-0295","310C-BCG-006-M3\nPost SB 31-0098","QAR201-02-00","2227000-85A","Custom -85A             64 wps","Type 1",null,"YES","Honeywell\nSteel","Internal",null,"1/1/1","UPGRADED","965-0976-003-236- 236",null,"Class A",null,null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","YES\nCollins","YES",null,"LH & RH\n822-1338-003",null,2015,"YES",null,null,null,null,null,"AAR\n55973-103","A, C, D, E","Available\n(56414-101)","Available\n(57305-102)","Available\n57305-102","Upper - E\nLower - C","K, P, Q","K, P, Q"]
[]
["315AA",null,"-223","BCSF","1985-02-15",22317,109,"VA511","CF6-80A","AAL",null,null,"ABX-3A","YES/180","YES","YES","YES",null,null,"SEE\nNOTE","A",352200,351000,283000,266000,"MTW/MTOW\n341800","YES","63-85 F (17-29.5 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)","40-50 F (4.5-10 C)",null,"YES","Rockwell Collins\nFCC-701, -702, -703","CH-EJ","YES","YES","YES\nCollins","ICG\nModel  ICS-220A\nP/N 710100-2","881623455799\n881623456202","Rockwell Collins\nCMU-900, 822-1239-151 (DEACT)","YES\n(Deact)",1,0,4,"Convection","No Door","YES","Portable\nHoneywell",null,"NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Simmonds\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","NONE","YES","317B-COL-DE0-08 POST SB 31-0295","310F-BCG-013-K2\nPost SB 767-34-0703","QAR201-02-00","2233000-816","767-3A\n256 wps","Type 1A",null,"NO","Honeywell\nCarbon","Internal",null,"5/15/5 DL","PENDING","965-0976-003-236- 236",475,"Class A",null,null,"4052506-955\nS242T102-455\nPegasus","OPS 3411-HNP-02C-10\nOPC 347F-BCG-01P-W8\nPost SB 34-701, 34-703","GB7","YES\nAvionics Group","YES",null,"LH & RH\n066-01127-1602","TCAS II 7.1\nAllied Signal\n(AAL)",2015,"YES",null,null,null,null,null,"AAR\n57700-103","A, C, D, E, F","Available\n(58242-101)","Installed\nConfig F","Installed\nConfig F","Upper - E\nLower - E","K, P, Q","K, P, Q"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NO (EFIS)"]
["313AZ","N337CM\nVH-OGH",-338,"BDSF","1990-12-19",24930,344,"VN088","CF6-80C2B6","QAN",null,null,"AMZ","YES/180","NO","YES","NO","NO",null,"SEE\nNOTE","D",381000,380000,320000,288000,"NONE",null,"60-84 F (19-29 C)\n37-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","LQ-BG","NO","YES","YES\nCollins","NO","NO","NO","NO",3,0,4,"Convection","No Door","YES","In Life Rafts",null,"YES",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.0 L","85200.0 LB\n38646.0 KG","Honeywell\nKG","SB\n767-28A0083","SB\n767-28A0085","YES","NO (EFIS)","YES","317B-COL-DE0-08 POST SB 31-0295"," 3104-BCG-01L-49\nPost SB 34-0611","QAR201-02-00","2233000-816","767-3A\n256 wps","Type 1A",null,"YES","Messier-Bugatti\nCarbon","External",null,"5/11/5 DL","PENDING","965-0976-020-236-236",478,"Class A",null,"822-1152-002\nw/GPS","4052506-955\nPegasus","OPS 3411-HNP-02C-10\nOPC 346A-BCG-01J-R2\nPost SB 34-605","GB7","YES","YES",null,"LH & RH\n7517800-1009","TCAS II 7.1\nCollins",2015,"YES",null,null,null,null,null,"AAR\n59400-104","A, C, D, E, F, G","Capable\n(59170-101)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, Q, A, L, M\nNo LD2","K, Q\nNo LD2","NO"]
["337AZ","N389CM\n N386AA",-323,"BDSF","1994-05-13",27060,540,"VN036","CF6-80C2B6","AAL",null,null,"AMZ","YES/180",null,null,null,"YES",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","NGS\nSB 767-47-0001",null,null,null,null,null,null,null,null,"NO"]
["353AZ","N384CM\n N371AA",-323,"BDSF","1992-05-07",25198,431,"VN021","CF6-80C2B6","AAL",null,null,"AMZ","YES/180",null,null,null,"NO",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","NO"]
["359AZ","N388CM\n N355AA",-323,"BDSF","1988-05-25",24036,221,"VN005","CF6-80C2B6","AAL",null,null,"AMZ","YES/180",null,null,null,"NO",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"317B-COL-DE0-08 POST SB 31-0295",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2015,null,"IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank","NO",null,null,null,null,null,null,null,null,"NO"]
["769AX","JA8481","-281","P2S","1983-06-01",22787,58,"VB103","CF6-80A","ANA",null,null,"DHL-1","NO","NO","NO","YES","NO",null,"SEE\nNOTE","C",312000,310000,272000,253000,"Minor aft CG\nRestriction",null,"66-77 F (19-25 C)\n36-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","BC-JM","NO","NO","NO","NO","N/A","NO","N/A",0,0,4,"Microwave","Standard","YES","Portable\nKannad",null,"NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","ADVISORY","YES","317B-COL-DE0-08 POST SB 31-0295","310B-BCG-00M-20\nPost SB 31-0098","N/A","2233000-816","767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"NO","N/A","965-0976-003-236-236",482,"Class A","No",null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","NO","YES",null,"LH 822-1338-002\nRH 066-01127-1301","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","IAI\nMonogram","IAI FWD Left\nBoeing Aft Deact","Lav Faucet Tank","NO","AAR\n55973-123","A, C, D, E, G","Available\n(56414-102)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["793AX","JA8241","-281","P2S","1985-04-25",23143,114,"VB117","CF6-80A","ANA",null,null,"DHL-1","NO","NO","NO","NO","NO",null,"SEE\nNOTE","C",312000,310000,272000,253000,"Minor aft CG\nRestriction",null,"66-77 F (19-25 C)\n36-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","AH-FL","NO","NO","NO","NO","N/A","NO","N/A",0,0,4,"None","Standard","YES","Portable\nKannad",null,"NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","ADVISORY","YES","317B-COL-DE0-08 POST SB 31-0295","310B-BCG-00M-20\nPost SB 31-0098","N/A","2233000-816","767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"NO","N/A","965-0976-003-236-236",483,"Class A","No",null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","NO","YES",null,"LH 822-1338-002\nRH 066-01127-1301","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","IAI\nMonogram","IAI FWD Left\nBoeing Aft Deact","Lav Faucet Tank","NO","AAR\n55973-103","A, C, D, E","Available\n(56414-101)","Available\n57305-102","Available\n57305-102","Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["794AX","JA8242","-281","P2S","1985-05-22",23144,115,"VB118","CF6-80A","ANA",null,null,"DHL-1","NO","NO","NO","NO","NO",null,"SEE\nNOTE","B",322000,319580,272000,258000,"MTW/MTOW\n315500",null,"66-77 F (19-25 C)\n36-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","AH-FM","NO","NO","YES\nHoneywell\nDEACTIVATED","AFIRS\nP/N 501-0001-1\nDEACTIVATED","N/A","NO","N/A",0,0,4,"None","Standard","YES","Portable\nKannad",null,"NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","ADVISORY","YES","317B-COL-DE0-08 POST SB 31-0295","310B-BCG-00M-20\nPost SB 31-0098","N/A","2233000-816","767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"NO","N/A","965-0976-003-236-236",488,"Class A","No",null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","NO","YES",null,"LH 822-1338-002\nRH 066-01127-1301","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","IAI\nMonogram","IAI FWD Left\nBoeing Aft Deact","Lav Faucet Tank",null,"AAR\n55973-123","A, C, D, E, G","Available\n(56414-102)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["775AX","JA8484","-281","P2S","1983-10-01",22790,69,"VB106","CF6-80A","ANA",null,null,"DHL-1","NO","NO","NO","NO","NO",null,"SEE\nNOTE","C",312000,310000,272000,253000,"Minor aft CG\nRestriction",null,"66-77 F (19-25 C)\n36-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","EK-CL","NO","NO","NO","NO","N/A","NO","N/A",0,0,4,"Microwave","Standard","YES","Portable\nKannad",null,"NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","NO (EFIS)","YES","317B-COL-DE0-08 POST SB 31-0295","310B-BCG-00M-20\nPost SB 31-0098","N/A","2233000-816","767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"NO","N/A","965-0976-003-236-236",601,"Class A","No",null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","NO","YES",null,"LH 822-1338-002\nRH 066-01127-1301","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","IAI\nMonogram","IAI FWD Left\nBoeing Aft Deact","Lav Faucet Tank",null,"AAR\n55973-123","A, C, D, E, G","Available\n(56414-102)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["787AX","JA8489","-281","P2S","1984-07-01",23020,96,"VB111","CF6-80A","ANA",null,null,"DHL-1","NO","NO","NO","NO","NO",null,"SEE\nNOTE","B",322000,319580,272000,258000,"MTW/MTOW\n315500",null,"66-77 F (19-25 C)\n36-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","EL-HJ","NO","NO","NO","NO","N/A","NO","N/A",0,0,4,"Microwave","Standard","YES","Portable\nKannad",null,"NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG AEROSPACE","NO","ADVISORY","YES","317B-COL-DE0-08 POST SB 31-0295","310B-BCG-00M-20\nPost SB 31-0098","N/A","2233000-816","767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"NO","N/A","965-0976-003-236-236",602,"Class A","No",null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","NO","YES",null,"LH 822-1338-002\nRH 066-01127-1301","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","IAI\nMonogram","IAI FWD Left\nBoeing Aft Deact","Lav Faucet Tank",null,"AAR\n55973-123","A, C, D, E, G","Available - See Note\n(56414-102)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["792AX","JA8240","-281","BDSF","1986-03-21",23142,110,"VB116","CF6-80A","ANA",null,null,"DHL-1","NO","NO","YES","NO","NO",null,"SEE\nNOTE","A",352200,351000,283000,266000,"NONE",null,"66-77 F (19-25 C)\n36-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","AH-FG","NO","NO","YES\nHoneywell","NO","N/A","NO","N/A",0,3,2,"Microwave","Boeing","YES","Portable\nKannad",null,"NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG AEROSPACE","NO","ADVISORY","YES","317B-COL-DE0-08 POST SB 31-0295","310B-BCG-00M-20\nPost SB 31-0098","QAR201-02-00","2233000-816","767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"NO","N/A","965-0976-003-236-236",601,"Class A","No",null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","NO","YES",null,"LH 822-1338-002\nRH 066-01127-1301","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","Boeing\nRogerson","Boeing AFT Active","Aircraft Press\nTank",null,"AAR\n55973-103","A, C, D, E","Available - See Note\n(56414-101)","Available\n57305-102","Available\n57305-102","Upper - E\nLower - C","K, P, Q","K, P, Q","YES"]
["788AX","JA8490","-281","P2S","1984-10-01",23021,103,"VB112","CF6-80A","ANA",null,null,"DHL-1","NO","NO","NO","NO","NO",null,"SEE\nNOTE","A",352200,351000,283000,266000,"NONE",null,"66-77 F (19-25 C)\n36-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","EP-DF","NO","NO","NO","NO","N/A","NO","N/A",0,0,4,"None","Standard","YES","Portable\nKannad",null,"NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG AEROSPACE","NO","NO (EFIS)","YES","317B-COL-DE0-08 POST SB 31-0295","310B-BCG-00M-20\nPost SB 31-0098","N/A","2233000-816","767-4\n64 wps","Type 1A",null,"YES","Honeywell\nSteel","Internal",null,"NO","N/A","965-0976-003-236-236",605,"Class A","No",null,"4052500-962         200k","PS4052520-162","GB3/4/5/6/9","NO","YES",null,"LH 822-1338-002\nRH 066-01127-1301","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","IAI\nMonogram","IAI FWD Left\nBoeing Aft Deact","Lav Faucet Tank",null,"AAR\n55973-123","A, C, D, E, G","Available - See Note\n(56414-102)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["798AX\n(Not in Service)","JA8251","-281","BDSF","1987-06-04",23431,143,"VB122","CF6-80A","ANA",null,null,"ABX-3B","NO","NO","NO","NO","NO",null,"SEE\nNOTE","A",352200,351000,283000,266000,"NONE",null,"66-77 F (19-25 C)\n36-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","AL-BJ","NO","NO","NO","NO","N/A","NO","N/A",0,3,2,"Microwave","Boeing","YES","Portable\nKannad","NO","NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","NO (EFIS)","YES",null,null,"N/A","2233000-816","767-4\n64 wps","Type 1A","NO","YES","Honeywell\nSteel","Internal","STANDARD",null,null,"965-0976-003-236-236",null,"Class A","No",null,"4052500-962         200k",null,"GB3/4/5/6/9","NO","YES","NO","LH 822-1338-002\nRH 066-01127-1301","TCAS II 7.1\nCollins",2015,"YES","Boeing - L1","Boeing\nEnvirovac","Boeing AFT Active","Aircraft Press\nTank",null,"AAR\n55973-103","A, C, D, E","Available - See Note\n(56414-101)","Available\n(57305-102)","Available\n(57305-102)","Upper - E\nLower - C","K, P, Q","K, P, Q","YES"]
["363CM","VH-OGF","-338","BDSF","1989-09-05",24853,319,"VN086","CF6-80C2B6","QAN",null,null,"ABX-2","YES/180","YES\n(NO ULD)","YES","NO","NO",null,"SEE\nNOTE","B",413000,412000,326000,309000,"MLW 320000\nMZFW 303000",null,"60-84 F (19-29 C)\n37-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","EK-DG","YES","YES","YES\nCollins","AFIRS\nP/N 501-0001-1","See PMI ACU\nTech Desc","NO","NO",3,0,4,"Convection","No Door","YES","In Life Rafts","NO","YES",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.0 L","85200.0 LB\n38646.0 KG","Honeywell\nKG","SB\n767-28A0083","SB\n767-28A0085","YES","NO (EFIS)","YES",null,null,"QAR201-02-00","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Messier-Bugatti\nCarbon","Internal","ESIS",null,null,"965-0976-020-236-236",null,"Class A","No",null,"4052506-941\nNPIP 1 MB",null,"GB8\n(US & Europe)","EHS\nEXT SQT","YES","YES","LH & RH\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank",null,"AAR\n59400-104","A, C, D, E, G, P","Available - See Note\n(59170-101)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, Q, A, L, M\nNo LD2","K, Q\nNo LD2","YES"]
["752AX","JA8255","-281","BDSF","1987-04-15",23434,171,"VB125","CF6-80A","ANA",null,null,"DHL-1","NO","NO","YES","NO","NO","ABX-ABX 767-200","SEE\nNOTE","A",352200,351000,283000,266000,"NONE",null,"66-77 F (19-25 C)\n36-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","DG-BK","NO","NO","NO","NO","N/A","NO","N/A",0,3,2,"Microwave","Standard","YES","Portable\nKannad","NO","NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","NO (EFIS)","YES",null,null,"uQAR","2233000-816","767-3A\n256 wps","Type 1A","NO","YES","Honeywell\nSteel","Internal","STANDARD",null,null,"965-0976-003-236- 236",null,"Class A","No",null,"4052500-962         200k",null,"GB3/4/5/6/9","EHS\nEXT SQT","YES","YES","LH 822-1338-002\nRH 066-01127-1301","TCAS II 7.1\nCollins",2015,"YES","Boeing - L1","Boeing\nEnvirovac","Boeing AFT Active","Aircraft Press\nTank",null,"AAR\n55973-103","A, C, D, E","Available - See Note\n(56414-101)","Available\n(57305-102)","Available\n(57305-102)","Upper - E\nLower - C","K, P, Q","K, P, Q","YES"]
["740AX","N101DA","-232","BDSF","1982-02-19",22213,6,"VA301","CF6-80A2","DAL",null,null,"ABX-1","NO","YES","YES","NO","NO","ABX-ABX 767-200","SEE\nNOTE","A",352200,351000,283000,266000,"NONE",null,"66-77 F (19-25 C)\n36-72 F (2-22 C)",null,"40-50 F (4.5-10 C)",null,"No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","LR-CH","YES","YES","YES\nHoneywell","NO","NO","NO","NO",0,3,2,"Microwave","Jamco","YES","Portable\nKannad","NO","NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG AEROSPACE","NO","ADVISORY","YES",null,null,"WQAR","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Honeywell\nSteel","Internal","ESIS",null,null,"965-0976-003-236-236",null,"Class A","No",null,"4052506-955\nPegasus",null,"GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","Boeing\nEnvirovac","Boeing AFT Active","Aircraft Press\nTank",null,"AAR\n55973-103","ABX Rapid Change\nRC1/RC2","ABX Rapid Change\nRC1/RC2","Available\n(57305-102)","Available\n(57305-102)","Upper - E\nLower - C","K, P, Q","K, P, Q","YES"]
["742AX","N105DA\nSE-RLC","-232","BDSF","1983-01-19",22217,27,"VA305","CF6-80A2","DAL",null,null,"Astrel","NO","NO","NO","Deactivated","NO","ABX-ABX 767-200","SEE\nNOTE","A",352200,351000,283000,266000,"NONE",null,"66-77 F (19-25 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)",null,null,"NO","Rockwell Collins\nModels FCC-701, -702, -703","LR-CM","YES","YES","YES\nHoneywell","ICG ICS-220A\nP/N 710100-2","Deactivated","Deactivated","Deactivated",0,3,2,"Microwave","Jamco","YES","Portable\nKannad","NO","NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","ADVISORY","YES",null,null,"N/A","2233000-816","767-4\n64 wps","Type !A","5/19/5 DL","YES","Honeywell\nSteel","Internal","ESIS",null,null,"965-0976-003-216-216\n221/53",null,"Class A",null,"822-1821-002\nw/GPS","4052506-955\nPegasus",null,"GB7","EHS\nEXT SQT","YES","YES","LH & RH\n822-1338-003","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","Boeing\nEnvirovac","Boeing AFT Active","Aircraft Press\nTank",null,"AAR\n55973-103","A, C, D, E\n55973-103","Available\n56414-101","Available\n57305-102","Available\n57305-102","Upper - E\nLower - C","K, P, Q","K, P, Q","YES"]
["749AX","N114DA","-232","BDSF","1984-01-25",22226,78,"VA314","CF6-80A2","DAL",null,null,"ABX-1","NO","YES","YES","YES","NO","\tABX-AMZ 767-200","SEE\nNOTE","A",352200,351000,283000,266000,"NONE",null,"66-77 F (19-25 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","LS-AF","YES","YES","YES\nHoneywell","ICG ICS-220A\nP/N 710100-2","881623455410\n881623455411","Rockwell Collins\nCMU-900, 822-1239-151","YES",0,3,2,"Microwave","Jamco","YES","Portable\nKannad","NO","NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","ADVISORY","YES",null,null,"WQAR","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Honeywell\nSteel","Internal","ESIS","5/11/5 DL",null,"965-0976-003-236-236",null,"Class A",null,"822-1821-002\nw/GPS","4052506-955\nPegasus",null,"GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","Boeing\nEnvirovac","Boeing AFT Active","Aircraft Press\nTank",null,"AAR\n55973-103","A, C, D, E","Available - See Note\n56414-101","Available\n57305-102","Available\n57305-102","Upper - E\nLower - C","K, P, Q","K, P, Q","YES"]
["795AX","JA8243","-281","P2S","1985-08-02",23145,116,"VB119","CF6-80A","ANA",null,null,"ABX-2","NO","NO","YES","NO","NO","ABX-AMZ 767-200","SEE\nNOTE","A",352200,351000,283000,266000,"NONE","YES","66-77 F (19-25 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","AK-EF","NO","NO","NO","NO","N/A","NO","NO",0,0,4,"Microwave","Standard","YES","Portable\nKannad","NO","NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG AEROSPACE","NO","ADVISORY","YES",null,null,"WQAR","2233000-816","767-3A\n256 wps","Type 1A","NO","YES","Honeywell\nSteel","Internal","STANDARD",null,null,"965-0976-003-236-236",null,"Class A",null,"No","4052500-955         Pegasus",null,"GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","IAI\nMonogram","IAI FWD Left\nBoeing Aft Deact","Lav Faucet Tank",null,"AAR\n55973-123","A, C, D, E, G","Available - See Note\n(56414-102)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["768AX","JA8480","-281","P2S","1983-05-01",22786,54,"VB102","CF6-80A","ANA",null,null,"ABX-4","NO","NO","NO","NO","NO","ABX-AMZ 767-200","SEE\nNOTE","767-2D",317000,315000,272000,253000,"Minor aft CG\nRestriction",null,"66-77 F (19-25 C)","36-72 F (2-22 C)","40-50 F (4.5-10 C)","40-50 F (4.5-10 C)","No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","AK-HS","NO","NO","NO","NO","N/A","NO","N/A",0,0,4,"None","Standard","YES","Portable\nKannad","NO","NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","ADVISORY","YES",null,null,"WQAR","2233000-816","767-3A\n256 wps","Type 1A","NO","YES","Honeywell\nSteel","Internal","STANDARD",null,null,"965-0976-003-236-236",null,"Class A",null,"No","4052506-955\nPegasus",null,"GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - Jamco\nL1","IAI\nMonogram","IAI FWD Left\nBoeing Aft Deact","Lav Faucet Tank",null,"AAR\n55973-123","A, C, D, E, G","Available - See Note\n(56414-102)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q","K, P, Q","N/A"]
["797AX","JA8245","-281","BDSF","1985-10-30",23147,123,"VB121","CF6-80A","ANA",null,null,"ABX-1A","NO","NO","YES","NO","NO","ABX-ABX 767-200","SEE\nNOTE","767-2A",352200,351000,283000,266000,"NONE","66-77 F (19-25 C)\nN/A, See Note",null,null,null,"40-50 F (4.5-10 C)","No AC System\n40-50 F (4.5-10 C)","NO","Rockwell Collins\nFCC-701, -702, -703","AK-FL","NO","NO","YES\nHoneywell","NO","N/A","NO","N/A",0,3,2,"Microwave","Boeing","YES","Portable\nKannad","NO","NO",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","4560.0 GAL\n17261.5 L","32376.0 LB\n14685.5 KG","Honeywell\nLB","TDG\nAEROSPACE","TDG\nAEROSPACE","NO","ADVISORY","YES",null,null,"WQAR","2233000-816","767-3A\n256 wps","Type 1A","NO (EFIS)","YES","Honeywell\nSteel","Internal","STANDARD",null,null,"965-0976-003-236-236",null,"Class A",null,"No","4052506-955\nPegasus",null,"GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","Boeing - L1","Boeing\nEnvirovac","Boeing AFT Active","Aircraft Press\nTank",null,"AAR\n55973-103","A, C, D, E","Available - See Note\n(56414-101)","Available\n(57305-102)","Available\n(57305-102)","Upper - E\nLower - C","K, P, Q","K, P, Q","YES"]
["372CM","VH-OGM",-338,"BDSF","1992-09-03",25575,451,"VN093","CF6-80C2B6","QAN",null,null,"DHL-1","YES/180","YES","YES","NO","NO","ABX-DHL 767-300","SEE\nNOTE","767-3E",381000,380000,320000,288000,"NONE",null,"60-84 F (19-29 C)","37-72 F (2-22 C)",null,null,"No AC System\n40-50 F (4.5-10 C)","YES","Rockwell Collins\nFCC-701, -702, -703","QR-AG","YES","YES","YES\nCollins","NO","NO","NO","NO",3,0,4,"Convection","No Door","YES","In Life Rafts","YES","YES",null,"6070.0 GAL\n22977.4 L","43097.0 LB\n19548.4 KG","12000.0 GAL\n45424.0 L","85200.0 LB\n38646.0 KG","Honeywell\nLB","SB\n767-28A0083","SB\n767-28A0085","YES","NONE","YES",null,null,"WQAR","2233000-816","767-3A\n256 wps","Type 1A","5/11/5 DL","YES","Messier-Bugatti\nCarbon","Internal","ESIS",null,null,"965-0976-020-236-236",null,"Class A",null,"822-1152-002\nw/GPS","4052506-955\nPegasus",null,"GB7","EHS\nEXT SQT","YES","YES","NXT-800\n9008000-10001","TCAS II 7.1\nCollins",2015,"YES","IAI - Dasell\nCockpit","IAI\nMonogram","IAI FWD Right\nBoeing Aft Deact","Lav Faucet Tank",null,"AAR\n59400-104","A, C, D, E, G, P","Available - See Note\n(59170-101)","Installed\nConfig G","Installed\nConfig G","Upper - E\nLower - C","K, P, Q, A, L, M","K, P, Q","YES"]
[]
[]
[]
[{"$f":"COUNTA(A6:A37)","v":30}]

{"sheet":"FIN","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}